QXDM Multi-platform Professional Release for Windows (Version 04.00.00270)

These Release Notes cover important information concerning Windows QXDM4 Professional

Table of Contents

1. Installation Notes
2. General Information
3. What's New in This Release?
4. Known Issues

-------------------------------------------------------------------------------

1. Installation Notes

Windows QXDM4 is built to run on Win7 and later Windows system. We also make it run on Windows XP at this point. But may drop the support for Windows XP in the future. 

QXDM Software Requirements:

Win7 and later Windows system.

Steps for regular Windows installation (to be used by internal users or external customers with internet access)

1)	Download the installer from Createpoint.
2)	Unzip the installer
3)	Double click on the install to install it. The default location is C:\Program Files (x86)\QUALCOMM\QXDM4

WINDOWS Installation Steps for External Customers Who has No Internet Connection
If you are external customers trying to install QXDM on a computer, called it ComputerA, without Internet access, please follow the steps below.

1)	On another Windows computer with Internet access, called it ComputerB, follow the Steps for Regular Installation above to install QXDM on it.
2)	On ComputerB, copy the installer and Qt5WebKit.dll to Computer A.
3)	On ComputerA, run the installer. Then copy the Qt5WebKit.dll into the folder C:\Program Files (x86)\QUALCOMM\QXDM4

-------------------------------------------------------------------------------

2. General Information

Please refer to The User’s Guide 

-------------------------------------------------------------------------------

3. What’s New

Latest QXDM Professional Software Version 04.00.00270 (7/10/2018).

•	New Features: None
•	Bug Fixes:
•	Automation
•	Fix for bug with GetItemName API
•	Displays
•	Fix for TDSCDMA Layer 1 display
•	Added support for v13 packets in GNSS Navigatiion Database display
•	DMC Updates: 
•	Default DMC version unchanged at version 10
•	Resolved following JIRA tickets:

JIRA	Title	Raised by	
QXDM-3830	TDS info miss on latest QXDM4-v.249	QCT QST MST Technologies BJ	
QXDM-3828	QXDM4.0.00.244 GetItemName() error	QCT Applications Engineering SH	

Latest QXDM Professional Software Version 04.00.00249 (6/5/2018).

Internal release with content equivalent to previous release. In addition:
•	New Features: None
•	Bug Fixes: None
•	DMC Updates: 
•	Default DMC version unchanged at version 10
•	Resolved following JIRA tickets: None

Latest QXDM Professional Software Version 04.00.00244 (5/30/2018).
•	New Features:
•	Automation
•	Added enhanced client APIs
•	Added APIs to replay an ISF
•	Displays
•	Added TSENS Dashboard display
•	Added support for v12 packets in GNSSNavigationDatabase and GNSSPositionReport displays
•	GUI
•	Enhancement to indicate log 0x19B6 needs to be enabled to collect QSH Metrics
•	Added "Accept Unknown" option to the config dialog
•	Parsing
•	Add Nr5G Rrc VF01 support
•	Other
•	Added quick disconnect feature
•	Bug Fixes:
•	Automation
•	Fixed a bug in NV Write from automation
•	Displays
•	Fixed the sorting in "Task Profiling - MPU" display
•	Fix to properly show SINR in "LTE ML1 Serving Cell" display
•	Fixes for "GPS Server" display
•	GUI
•	Fix to make Log View window position persistent
•	Pin the Progess Dialog to the location where it was first created
•	Item View / Filtered View
•	Improved efficiency for match
•	Fix to display summary field for several GPS logs
•	Parsing
•	Improved robustness when parsing malformed packets
•	Other
•	Changed copy shortcut from Alt+C to Ctrl+C
•	Fixed Ctrl+N to skip to the next matching record
•	DMC Updates: 
•	Default DMC version unchanged at version 10
•	Resolved following JIRA tickets:
JIRA	Title	Raised by	
QXDM-3431	Quick COM disconnect	Internal	
CTAHELP-35373	NV write is not going through on Meta-152 Job SDX_SS_V4_MN	QCT Product & Tools SW I&T SD	
QXDM-3438	Add additional COM API Functionality	Internal	
QXDM-3249	TSENS QXDM Dashboard	QCT Core Technologies Wired Connectivity SW SD	
QXDM-3546	'Task Profiling - MPU' issue in QXDM4.0.226	QCT Applications Engineering SH	
QXDM-3563	Window customization	QCT QST MST Commercialization GRMNY	
QXDM-3448	QSH metric logging fine tune	QCT Modem SW - MMCP SD	
QXDM-3615	Change shortcut key from Alt+C to "Ctrl+C"	QCT Modem SW - LTE BJ 	
QXDM-3616	Implement CTRL + N	QCT Modem SW - LTE BJ	
QXDM-3658	Find Next Dialog Movement	ASW	
QXDM-3613	GNSS Navigation Database display enhancement 0x147B v12	QCT Location Technology SCL	
QXDM-3639	QXDM display enhancement for DM log GNSS position report - 0x1476 version 12	QCT Location Tech- Bangalore	
QXDM-3648	Add Summary for Several GPS Logs	QCT Location Technology SCL	
QXDM-3408	RE: issue about QXDM4 diag mask for subsystem packet	Internal	
QXDM-3679	QXDM 04.00.230 can not show SINR	Internal	
QXDM-3518	GPS Server Window misbehaving 	QCT WT EngOps Applications Engineering HYD	

Latest QXDM Professional Software Version 04.00.00230 (3/29/2018).
•	New Features:
•	Automation APIs
•	Implemented ConfigureClientByName api
•	
•	DBs
•	Updated OneWeb event 2948
•	Added "LTE ML1 Sleep" (0xB18B) version 33 packet
•	Add TSENS Packets
•	Added "LTE UE Identification Message (MSG3) Report" (0xB169) version 3 packet
•	Updated OneWeb 0xB465, 0xB460
•	Updated QMI UIM from the latest aml
•	Add following 10 new messages:
QMI_NAS_V2X_NOTIFICATION (197)
QMI_NAS_SET_ECID_CONFIG (201)
QMI_NAS_GET_ECID_CONFIG (202)
QMI_NAS_SUB_BLOCKED_STATUS (203)
QMI_NAS_GET_SUB_BLOCKED_STATUS (204)
QMI_NAS_LTE_B2_THRESH_ADJ_CONFIG (205)
QMI_NAS_V2X_START (206)
QMI_NAS_V2X_STOP (207)
QMI_NAS_GET_V2X_STATUS (208)
QMI_NAS_V2X_NOTIFICATION (209)
•	Added "LTE LL1 Serving Cell TTL Results" (0xB11D) version 141 packet
•	Added event "EVENT_LTE_ELS_MCE_BUILD" (3145)
•	Added new "LTE RRC Cap Related Info" (0xB0D1) version 32 packet
•	Added "TBS PDCCH Tx Report" (0x9404) , "TBS PDCCH Tx Debug Report" (0x9405), "TBS PUSCH Rx Report" (0x9406), "TBS SRS Rx Report" (0x9408)
•	Added "LTE LL1 PUSCH Tx Report" (0xB139), "LTE LL1 PUCCH Tx Report" (0xB13C) and "LTE LL1 SRS Tx Report" (0xB140) Version 141 packets
•	Added "MSG_SSID_MCS_TRM" (4616)
•	Added "LTE LL1 CSF Spectral Efficiency TxMode 1, 2, 7" (0xB14B) version 141, "LTE PRACH Configuration" (0xB166) version 40 and "LTE Random Access Request (MSG1) Report" (0xB167) version 40 packets
•	Add WCDMA X2W List Search Results (0x41D9) version 3 packet
•	Added following events:
EVENT_WLAN_FW_CONN_MGMT_SEND_V2  [3156]
EVENT_WLAN_FW_CONN_MGMT_RECV_V2 [3157]
EVENT_WLAN_FW_CONN_MGMT_SSID [3159]
•	Added WCDMA Slot Level ILPC Debug Log Packet (0x4778) Version 5
•	Created 0x4179 V11 , V12 and 0x4177 V8
•	Added "OW MAC Statistics Summary" and "OW PDSCH HARQ Id Histograms" analyzers
•	Added OW ML1 WARM START INFO (0xB5E1)
•	Added OW ML1 MQA Information (0xB5E2)
•	Added OW RRC OW SATELLITE ACQUISITION INFO (0xB4CE)
•	Added OW LL1 Time Sync search Results (0xB515)
•	Added OW LL1 PSS-RS Search Results (0xB513)
•	Add ADSP PCM packets (0x19AF, 0x19B0, 0x19B1) to vocoder playback support
•	Added following 6 new messages:
QMI_VOICE_GET_SPEECH_CODEC_INFO (112)
QMI_VOICE_IMS_CALL_CANCEL_OPERATION (113)
QMI_VOICE_AVOID_PLMN_LIST (114)
QMI_VOICE_SET_ECALL_OPRT_MODE (115)
QMI_VOICE_GET_ECALL_OPRT_MODE (116)
QMI_VOICE_ECALL_OPRT_MODE_IND (117)
•	Updated following 18 messages based on QMI VOICE spec 2.101:
QMI_VOICE_INDICATION_REGISTER (03)
QMI_VOICE_GET_CALL_INFO (36)
QMI_VOICE_ALL_CALL_STATUS_IND (46)
QMI_VOICE_GET_ALL_CALL_INFO(47)
QMI_VOICE_SET_SUPS_SERVICE (51)
QMI_VOICE_GET_CALL_WAITING (52)
QMI_VOICE_GET_CALL_BARRING (53)
QMI_VOICE_GET_CLIP (54)
QMI_VOICE_GET_CLIR (55)
QMI_VOICE_GET_CALL_FORWARDING (56)
QMI_VOICE_SET_CALL_BARRING_PASSWORD (57)
QMI_VOICE_ORIG_USSD (58)
QMI_VOICE_USSD_IND (62)
QMI_VOICE_GET_COLP (75)
QMI_VOICE_GET_COLR (76)
QMI_VOICE_GET_CNAP (77)
QMI_VOICE_MANAGE_IP_CALLS (78)
QMI_VOICE_MODIFIED_IND (81)
•	Enhanced "NR5G PUSCH Summary" and "NR5G PDSCH Summary" with new stats
•	Added "LTE LL1 PDSCH Decoding Results" (0xB132) version 142 and "LTE ML1 Intra Frequency Cell Reselection" (0xB181) version 25 packets
•	Added "LTE RLC DL UM Data PDU" (0xB086) and "LTE RLC UL UM Data PDU" (0xB096) version 4 packets
•	Add following log Ids:
IMS ICS Static Config  (0x1C40)
IMS ICS User Settings (0x1C41)
IMS ICS PM Config (0x1C42)
IMS ICS Network Conditions (0x1C43)
IMS ICS TRM (0x1C44)
IMS ICS NW Connectivity (0x1C45)
IMS ICS Timer (0x1C46)
IMS ICS Measurements (0x1C47)
IMS ICS Call States (0x1C48)
IMS ICS PDN State (0x1C49)
•	Added "V2X PDCP TX Data PDU" (0xB2D8) Version 2, "V2X PDCP RX Data PDU" (0xB2D9) Version 2 and "V2X PDCP TX Discard Data PDU" (0xB2DA) Version 2 packets
•	Added "LTE ML1 Multisim" (0xB182) version 40 and "LTE LL1 RX Antenna Info" (0xB15B) version 141 packets
•	Added "V2X DS" (0xB2E8) version 2 packet
•	Added "LTE ML1 Multisim Packet" (0xB182) version 28 packet
•	Added TRM (0x12E8) V18
•	Add Support for 7 Carriers for following log packets:
LTE PDSCH Stat Indication (0xB173) Version 37
LTE ML1 AdvRx IC Cell List (0xB18F) Version 35
LTE ML1 AdvRx IC Request (0xB190) Version 2
•	Added "LTE LL1 Multi RAT DL Report" (0xB13A) Version 141 packet
•	Added  7CA Support to following log packets:
LTE ML1 Neighbor Cell Meas Request/Response (B192) Version 1
LTE ML1 Serving Cell Meas Response (B193) Version 1
LTE ML1 Search Request/Response (B194) Version 1
LTE ML1 Connected Neighbor Meas Request/Response (B195) Version 1
•	Added ML1 Gen Log packets' following new sub packets ids
"Serving Cell Info" (Sub Id 16) Version 24
"Measurement ID Configuration" (Sub Id 17) Version 25
"Measurement Object Configuration" (Sub Id 18) Version 24
"Reporting Configuration" (Sub Id 19) Version 25
"Quantity Configuration" (Sub Id 20) Version 24
"Measurement Gap Configuration" (Sub Id 21) Version 24
"s-Measure Configuration" (Sub Id 22) Version 24
"Neighbor Cell Configuration" (Sub Id 23) Version 24
"Speed-Dependent Scaling Parameters" (Sub Id 24) Version 24
"Conn Meas Config Bitmasks" (Sub Id 37) Version 24
•	Add 7CA Support to packet LTE LL1 CSF Adaptation(0xB147) Version 127
•	Added packet OW LL1 Serving Cell measurements Info (0xB522) Version 1
•	Added missing packets into OTA Types
•	Displays
•	Add new 5G display for Filtered Cell BRSRP
•	Add OwMACConfig display
•	Added new display GNSS Primary RF Status
•	Add TSENS display
•	Add One web LL1 PUSCH PHY Throughput display
•	Add One web Rlc Config display
•	Add One web Pdcp Config  display
•	NV
•	Added new EFS NV item 74070
•	Added EFS NV Item 74071
•	Added EFS NV Item 74072
•	Added new EFS NV items 74073,74074
•	Added new EFS NV Items 74075,74076
•	Added new EFS NV Items 74073,74077,74078
•	Added New EFS NV Items 74079-74081
•	Added EFS NV items 74082-74086
•	Added new EFS items 74087, 74088
•	Added new EFS items 74089-74091
•	Parsing
•	Updated third party TRM parser to V18
•	Other
•	Mbn Viewer to display the contents of mbn file and delta xml
•	Bug Fixes:
•	Automation APIS
•	Fixed for Filtered View when created from automation
•	Allow Automation Debug logs to be disabled
•	Provided script support to open AutomationWindow2 in invisible mode
•	DBs
•	Updated OneWeb 0xB465, 0xB460
•	Updated the QMI NAS service from latest QMi Spec, QMI_MCS_QCSI_PKT (0x1544)
•	Updated following 15 messages with new TLVs:
QMI_NAS_INDICATION_REGISTER (03)
QMI_NAS_PERFORM_NETWORK_SCAN (33)
QMI_NAS_GET_RF_BAND_INFO  (49)
QMI_NAS_SET_SYSTEM_SELECTION_PREFERENCE (51)
QMI_NAS_GET_SYSTEM_SELECTION_PREFERENCE (52)
QMI_NAS_GET_SYS_INFO (77)
QMI_NAS_SYS_INFO_IND (78)
QMI_NAS_UPDATE_IMS_STATUS (114)
QMI_NAS_PERFORM_INCREMENTAL_NETWORK_SCAN (133)
QMI_NAS_SSAC_CHANGE_INFO_IND (144)
QMI_NAS_SET_DRX_SCALING_FACTOR (159)
QMI_NAS_GET_RPM_PARAMETERS (170)
QMI_NAS_GET_LTE_CPHY_CA_INFO (172)
QMI_NAS_GCELL_INFO_IND (188)
QMI_NAS_EDRX_CHANGE_INFO_IND (191)
•	Update OW PDSCH Stat Indication(0xB573) Version 2
•	Updated OW PDCP DL Cipher Data PDU (0xB4A3) Subpacket Version 2
•	Updated OW PDCP UL Cipher Data PDU (0xB4B3) Subpacket Version 1
•	Update EVENT_OW_MAC_RESET_V2 (2982)
•	Update OW LL1 PDCCH Decoding Result (0xB530) Version 7
•	Update OW LL1 PDCCH Decoding Result (0xB530) Subpkt v7
•	Update OW LL1 Periodic CSF(0xB54D) log packet name change
•	Update OW LL1 Aperiodic CSF(0xB54E) log packet name change
•	Update OW PDCP DL Reordering Stats (0XB4A6) modified bitmap representation
•	Fixed OW LL1 Time Sync search Results (0xB515) V1
•	Fixed OW LL1 PSS-RS Search Results (0xB513) V1
•	Update LTE PDSCH Stat Indication (B173) Version 36 for 7CA support
•	Update EVENT_OW_RRC_TIMER_STATUS (2906)
•	Update 0xB063 subpkt 7 for carrier index
•	Fixed 0xB16C Version 28 DAI field
•	Displays
•	Changes to show scc information correctly in LTE ML1 Serving Cell Measurements Display
•	Fixes for user plots
•	Fixes for "WCDMA HSDPA Link Statistics" and "UMTS Cell Reseleciton" displays
•	Fixes for PMIC ADC Dashboard
•	Add CDSP component into Ulog General View
•	Fixes for BDS measurement and GAL measurement displays
•	Fixes to support SCC4 in LTE ML1 displays
•	Fix for incorrect values showing in Lte ML1 Serving Cell Measurement display
•	Fix for Task Profiling MPU display
•	GUI
•	Fixes for Diag-ULog functionality
•	Fix the MessageBox popout issue for "Wrong Present QShrink4 File in the device"
•	Item View / Filtered View
•	Fixes for custom colors in Item View and Filtered View
•	Add color over ride color items to Filterview
•	NV
•	Fixes for EFS NV items 73942,73943
•	Updated EFS NV Item 72509
•	Updated EFS NV Items 73835,73846
•	Updated EFS NV Item 65882, 70326
•	Edited EFS NV Items 73880,73842,71556
•	Edit EFS NV Item 73683
•	Modify the NV item 72627
•	Fix for NV in case of multi-sim device
•	Fix for NV issue in case of automation
•	Parsing
•	Fixed parsing of E-ARFCN
•	Other
•	Fix for bug with replay
•	Fix the timestamp bug in the QTrace Message packet
•	Fix for wait in Command Interface API
•	DMC Updates: 
•	Default DMC version updated to version 10:
•	Most QTraces added to Default DMC
•	Resolved following JIRA tickets:
JIRA	Title	Raised by	
QXDM-3342	QXDM4 stopped during auto-test	QCT QST MST Technologies BJ	
QXDM-3363	RegisterClient() not work in WCDMACall.p	QCT Applications Engineering SH	
QXDM-2884	QXDM4 automation script: QXDMConfigureClientByNames.pl run failed	QCT Applications Engineering SH	
QXDM-3461	Automation Logs are blowing out the file system	Israel Modem Tech Engineering Mgmt	
QXDM-3412	Please provide review support for Perl script using QXDM API"s	QCT SW CE EngOps HYD	
QXDM-3500	Latest dll with support for TRM v18	QCT Modem SW - MCS HYD	
QXDM-3019	Request to add new QXDM display - Pre5G Filtered Cell BRSRP Plot (FR 46385)	QCT QST MST Technologies SD	
QXDM-3251	Add TSENS Packets to Diag DB	QCT Core Technologies Wired Connectivity SW SD	
QXDM-3331	No SCC info for LTE ML1 Serving Cell Measurements Display	QCT SW CE EngOps TWN	
QXDM-3265	Filtering of diagbuffers	Diag team	
QXDM-3210	Requirement to generate 5G histogram throughput for each carrier in single plot.	CORP ENG - Corporate Product Test	
QXDM-3172	QXDM display: MAC Config	QCT Software Target Program Management	
QXDM-3374	WCDMA Pilot Scanner forces itself to stay active in foreground/does not reliably populate	QCT QST MST Commercialization SD	
QXDM-3294	PMIC ADC Dashboard - export all samples on graph	QCT Core Technologies Wired Connectivity SW SD	
QXDM-3308	CDSP under ULog viewer	QCT Core Technologies DSP Performance HYD	
QXDM-3388	QXDM4 No RFSTATUS for GEN8B	QCT Location Technology SCL	
QXDM-3311	Re: tst_Dynamic _Status _Static _Status_Replay fail	Internal	
QXDM-3362	Adjust color for each QXDM item	QCT Applications Engineering SH	
QXDM-3249	TSENS QXDM Dashboard	QCT Core Technologies Wired Connectivity SW SD	
QXDM-3424	Observing QShrink as well as Logging issue on QXDM v221	QCT QST MST Technologies HYD	
QXDM-3447	Power up logs using Qtrace	QCT Modem SW - MMCP SD	
QXDM-3454	QXDM shows incorrect E-ARFCN in Filtered View logs	QCT SW CE EngOps HYD	
QXDM-3460	Change the BDS measurement and GAL measurement window to new IDs	QCT Location Tech- Bangalore	
QXDM-3457	no SCC4 data for LTE ML1 views	QCT SW CE EngOps TWN	
QXDM-381	LTE ML1 Serving Cell Measures Display	QCT SW CE EngOps TWN	
QXDM-348	Adjust color for each QXDM item is not working for Filter Views	QCT Applications Engineering SH	
QXDM-3489	Unable to schedule NVRead request for NVItem - 74 :: auto_answer	MST	
QXDM-3502	Delays in scr scripts are not executed in latest QXDM 227 version	QuIC Core Technologies Software Services SW HYD	
QXDM-3488	Limitations to GSM OTA logging in QXDM4	QCT SW CE EngOps HYD	
QXDM-3546	'Task Profiling - MPU' issue	QCT Applications Engineering SH	
CTAHELP-35373	NV write is not going through on Meta-152 Job SDX_SS_V4_MN	QCT Product & Tools SW I&T SD	

Latest QXDM Professional Software Version 04.00.00226 (2/13/2018).

•	New Features:
•	Automation APs
•	Added new automation APIs for retrieving field values by position
•	GUI
•	Added support for user defined item colors
•	Bug Fixes:
•	Displays
•	Fixes for bugs in WCDMA Pilot Scanner, WCDMA HSDPA Link Statistics, and UMTS Cell Reselection displays
•	GPS
•	Fixed GPS Server Info Display
•	DMC Updates: 
•	Default DMC version unchanged at version 9
•	Resolved following JIRA tickets:
JIRA	Title	Raised by	
QXDM-3405	GPS Server Info is missing	QCT SW CE EngOps HYD	
QXDM-3374	QXDM logging Issue for WCDMA/3G Logs	QCT QST MST Commercialization SD	
QXDM-3322	QXDM4 BUG (CRATFT) - WCDMA Pilot Scanner forces itself to stay active in foreground/does not reliably populate	QCT QST MST Commercialization SD	
QXDM-3362	Adjust color for each QXDM item	QCT Applications Engineering SH	

Latest QXDM Professional Software Version 04.00.00220 (1/10/2018).
•	New Features:
•	Automation APIs
•	Added 3 new automation interfaces API: AddSubsysV2Request, AddSubsysV2ImmediateResponse, AddSubV2DelayedResponse
•	SetSearchString api not working when used twice in script
•	DBs
•	Added following packets' new versions:
"LTE LL1 CSF SE TM9 Results" (0xB138) Version 141
"LTE LL1 CSF CSIRS Chest TM9" (0xB148) Version 141
"LTE LL1 PUCCH CSF" (0xB14D) Version 141
"LTE LL1 PUSCH CSF" (0xB14E) Version 141
•	Added "GSM Antenna Switch Diversity" (0x508A) and  "GSM DSDS Antenna Switch Diversity" (0x5A8A) version 2
•	Added following new versions
"LTE PDCP DL Ctrl PDU" (0xB0A2) Version 40 
"LTE PDCP DL Cipher Data PDU"  (0xB0A3) Version 40
"LTE PDCP DL SRB Integrity Data PDU" (0xB0B5) Version 40
"LTE PDCP UL Ctrl PDU" (0xB0B2) Version 40
"LTE PDCP UL Cipher Data PDU"  (0xB0B3) Version 40 
"LTE PDCP UL SRB Integrity Data PDU" (0xB0B5) Version 40
•	Added "OW LL1 PUSCH CSF" (0xB54E) version 1
•	Added the following LTE Band Enums to "LTE RRC Idle Meas Config Info" (0xB0C8) V2:
SYS_SBAND_LTE_EUTRAN_BAND46 = 45
SYS_SBAND_LTE_EUTRAN_BAND47 = 46,
SYS_SBAND_LTE_EUTRAN_BAND48 = 47,
SYS_SBAND_LTE_EUTRAN_BAND66 = 65,
SYS_SBAND_LTE_EUTRAN_BAND71 = 70,
SYS_SBAND_LTE_EUTRAN_BAND250 = 249
•	Updated V2 for packet 1C02 (NR5G Profiling)
•	Added "LTE LL1 PUCCH Tx Report" ( 0xB13C) Version 122
•	Added "LOG_GNSS_BDS_B2_MEASUREMENT_REPORT_C 0x1923" and "LOG_GNSS_GAL_E5A_MEASUREMENT_REPORT_C 0x1924"
•	Added "TLM CellDB Record 0x14FD" Version 10
•	Created 5 LTE RRC CGI Events 3139 to 3143
•	Added "TLM CellDB Record 0x14FD" Version 10
•	Updated 2914 OW event
•	Added "OW PDCP DL Reordering stats" (0xB4A6) V1
•	Parsing added for "0x1C4A" MC Clock Voting status
•	Added "LTE LL1 PDSCH Decoding Results" (0xB132) Version 141
•	Added "LTE RRC Supported CA Combos" (0xB0CD) Version 40
•	Created 5 new CGI events 0x3139 to 0x3143
•	Added "LTE LL1 PSS Results" (0xB113) V141
•	Update PDCP 0xB4B4 packet
•	Added following packets' new versions:
"LTE DCI Information Report" (0xB16C) Version 10
"LTE GM TX Report" (0xB16D) Version 10
"LTE PDSCH Stat Indication" (0xB173) Version 18
•	Update OW B4A6 packet
•	Added QDR2 changes "QDR Sensor Data(0x1957)"
•	Update OW 0xB460 packet
•	Added "IMS RTP SN and Payload" (0x1568) Version 11
•	Added SV Bit mask changes "GNSS ME Clock Voting Status (0x1C4A)"
•	Added "LTE LL1 Neighbor Cell Measurements and Tracking" (0xB119) Version 141 and "LTE LL1 PBCH Decoding Results" (0xB12E) Version 141 packets
•	Added "IMS RTP SN and Payload" (0x1568) Version 12 packet
•	Update V2X 0xB282 V7
•	Update OW 0xB4A6 packet
•	Update OW event 2906 and 2948
•	Displays
•	Added rows for scell3 in table  for LTE ML1 Serving Cell Measurement rssi sinr display
•	Added new html QXDM display - Pre5G Acquisition and Rach Stats
•	Added CV2X Activity Display
•	Add new 5G displays for DL throughput and BLER
•	Add new 5G displays for UL throughput and BLER
•	GUI
•	Added one click refresh all views in menu to replay isf with no delay (Silent Replay Dialog)
•	NV
•	Added EFS NV Items 74054-74057
•	Added New EFS NV Items 74058,74059
•	Added EFS NV Items 74060,74061
•	Added EFS NV Item 74062
•	Added new EFS NV Items 74063, 74065, 74066
•	Added EFS NV Items 74067-74068
•	Added EFS NV Item 74069
•	SILK
•	Updated the TS24.008 to VE30
•	Generated CSN.1 definition from 24.008
•	Added Extended protocol configuration options (e-PCO) IE
•	Added e-PCO IE to following messages
Activate PDP contect reject
Request PDP context activation
Request PDP context Activation reject
Modify PDP context request (Network to MS)
Modify PDP context request (MS to Network)
Modify PDP context accept (MS to Network)
Modify PDP context accept (Network to MS)
Modify PDP context reject
Deactivate PDP context request
Deactivate PDP context accept
•	Other
•	Added link to user guide in Help dropdown
•	Bug Fixes:
•	DBs
•	Fixed 0xB173 "ACK/NACK Decision"
•	Updated "OW LL1 PUCCH CSF" (0xB54D)
•	Fixed "QMI_PDS_INJECT_SPEED_DATA" (142) Speed (2) Tlv
•	Fixed "QMI_PDS_INJECT_COURSE_OVER_GROUND_DATA" (102) message
•	Changed Version20 to V20 "QDR Diag PKTs 0x195D,0x195E etc"
•	Displays
•	Fetch correct type of EARFCN data from DB
•	Add UI in general setting to define the plot font size
•	Fix the bug which the label didn't get update when set the font
•	Add display under right category and remove number printed on axis
•	Display antenna data individually in LTE ML1 Serving Cell Measurements Display
•	Fix for some displays like WCDMA Pilot Scan missing the Context menu for M-Sim and Show Packets
•	GPS
•	Use system default settings for comm ports
•	GUI
•	Verify that line has something in it before writting.  Strip off white space around fields
•	NV
•	Edited EFS NV Item 73764
•	Edited EFS NV Items 67330,73713
•	Edited EFS NV Item 67332
•	Edited EFS NV Item 67348, 72589
•	Updated EFS NV Item 73581
•	Parsing
•	Fix parsing of LTE OTA log parsing issue for Multefire
•	QDSS
•	Fix for QDSS HW timestamp issue
•	Fix for QDSS enable/disable not working via automation APIS
•	Fixed Diag over QDSS issue that hardware timestamp didn't shown for QDSS with multi-sim packets.
•	
•	SILK
•	Fixed the field length of DDX in ESM data transport
•	Fixed the parsing issue for PDN Address Information IE
•	Other
•	Fix QuitApplication() api, as user was not able to create another object of QXDM after calling QuitApplication()
•	Fixed a high CPU usage of QXDM issue when QXDM started
•	Disable hide/unhide columns feature in the command output window.
•	Add decoded ssId and ssMask for the post-processing error formated decoded message packets
•	DMC Updates: 
•	Default DMC version unchanged at version 9
•	Resolved following JIRA tickets: 
JIRA	Title	Raised by	
QXDM-3202	HW time stamp is NOT generated even QDSS logging is started	QCT QST MST Commercialization JPN	
CTAHELP-34958	Configure Automation for DIAG over QDSS	QCT QST MST Technologies HYD	
QXDM-3269	QXDM instance is not able to create for second time in QXDM4 version 04.00.211	QCT Auto APT BDC	
QXDM-3241	QXDM4 Process Consuming around 30% of CPU even in Disconnected mode	QCT SW CE EngOps HYD	
QXDM-3267	QXDM4.00.210 would occupy CPU 100%	QCT Applications Engineering SH	
QXDM-3316	QXDM API's based script not working after upgrading to latest qxdm ver 210	QCT SW CE EngOps HYD	
QXDM-3297	RE: Configure Automation for DIAG over QDSS	QCT Core Technologies Software Services SW HYD	
QXDM-3006	FR 46016: Add Scell3 to "LTE ML1 Serving Cell Measurements Display” and release data 11/17/17	QCT Software Target Program Management	
QXDM-2861	Can't unhide(restore) the contents of command output after hide them	China CE	
QXDM-3056	Request to add new QXDM display - Pre5G Acquisition and Rach Stats	QCT QST MST Technologies SD	
QXDM-3138	Does AddSubsysV2ImmediateResponse and AddSubsysV2DelayedResponse available	Internal	
QXDM-3166	CV2X displays	Internal	
QXDM-3214	LTE OTA log parsing issue for Multefire	Internal	
QXDM-3127	QXDM is not showing the right EARFCN whereas Apex is showing	QCT QST MST Commercialization SD	
QXDM-2811	Add "refresh all views" option under "File" menu	Qualcomm Reference Design QRD	
QXDM-3163	Font size for table window	QCT SW CE EngOps TWN	
QXDM-2982	Request to add new QXDM displays - DL Throughput and BLER(FR 45743)	QCT QST MST Technologies SD	
QXDM-2983	Request to add new QXDM displays - UL Throughput and BLER(FR 46097)	QCT QST MST Technologies SD	
QXDM-3013	Request to add new QXDM display - Pre5G RRC State Change Plot (FR 46355)	QCT QST MST Technologies SD	
QXDM-2973	New line inserted when copying the F3	QCT QST MST Commercialization SD	
QXDM-3306	RE: NEW Issue Record IR-264336 has been entered. The payload of DLF logging based on QMSL is incorrect comparing with QXDM logging	QCT IoE Applications Engineering SZ	
QXDM-3270	QXDM 0xB193 LTE ML1 Serving Cell Measurements Display	QCT SW CE EngOps TWN	
QXDM-3299	Some displays like WCDMA Pilot Scan missing the Context menu for M-Sim and Show Packets	QCT Product & Tools SW Analytics & Global Automation SD	

Latest QXDM Professional Software Version 04.00.00210 (11/20/2017).
•	New Features:
•	Automation APIs
•	Added automation api for adding qsh metrics packets
•	Added new Automation API to return current Rx Rate
•	DBs
•	Add "UL HS DPCCH Information Log Packet Edition 2" (0x421C) v4 and "HS-SCCH Decode Status with data" (0x423F) v3
•	Added "LTE LL1 PUCCH CSF" (0xB14D) version 103 and "LTE LL1 PUSCH CSF" (0xB14E) version 103
•	Added events "LTE_SCELL_CONFIGURATION_V2" (2887) and "LTE_SCELL_ACT_DEACT_CMD_V2" (2888)
•	Added "TDSCDMA FW RFC Slot Update" (0xD12E) Version 122 packet
•	Added "LTE ML1 Serving Cell Meas Response" (0xB193) sub packet 25 version 36
•	Added QMI_PDS_SET_E911_OVERRIDE_CONFIG (0x00A9) and QMI_PDS_GET_E911_OVERRIDE_CONFIG (0x00AA) messages
•	Added  "GNSS GTS log packets" (0x18AB version 7, 0x18AC version 1, 0x18AD version 4, 0x18AE version 4)
•	Added "LTE RLC DL Config Log packet" (0xB081) version 3
•	Added "MSG_SSID_GNSS_HLOS"  (121) Message
•	 Added "OW LL1 PDCCH Decoding Result" (0xB530) version 7, "OW LL1 PDSCH Decoding Results" (0xB532) version 4
•	Added "LTE ML1 Cell Measurement Results" (0xB196) Version 33
•	Added "OW ML1 Handover Information" (0xB5E0) Version 1
•	Added  following 8 new versions packets:
"OW MAC Config" (0xB460) Version 2
"OW PDCP DL Config" (0xB4A0) Version 2
"OW PDCP DL Cipher Data PDU" (0xB4A3) Version 2
"OW PDCP DL Statistics" (0xB4A4) Version 2
"OW PDCP UL Config" (0xB4B0) Version 2
"OW PDCP UL Statistics" (0xB4B4) Version 2
"OW RLC DL Config" (0xB481) Version 2	
"OW RLC UL Config" (0xB491) Version 2
•	Added following 6 new messages:
QMI_UIM_SET_APDU_BEHAVIOR (107)
QMI_UIM_PROFILE_USER_CONSENT (108)
QMI_UIM_EUICC_DEFAULT_SERVER_ADDRESS (109)
QMI_UIM_MAP_PROVISIONING_SESSIONS_TO_SLOTS (110)
QMI_UIM_READ_BER_TLV (111)
QMI_UIM_READ_BER_TLV_LONG_IND (112)
•	Added "LTE LL1 Serving Cell CER" (0xB122) version 142
•	Added "TDSCDMA FW RFC Slot Update" (0xD12E) version 123 packet
•	Added "ROCH TCP Compressor" (0x19E7) Version 2
•	Added "LTE RF FED Tx AGC " (0x184C) Version 8
•	Added "TRM" (0x12E8) Version 17
•	Added "LTE LL1 PSS Results" (0xB113) version 23
•	Added "LOG_GNSS_INJECT_SENSOR_DATA" (0x1510) Version 3
•	Added following new messages:
QMI_LOC_EVENT_FDCL_SERVICE_REQ_IND
QMI_LOC_GET_FDCL_BS_LIST_REQ
QMI_LOC_GET_FDCL_BS_LIST_RESP
QMI_LOC_GET_FDCL_BS_LIST_IND
QMI_LOC_INJECT_FDCL_DATA_REQ
QMI_LOC_INJECT_FDCL_DATA_RESP
QMI_LOC_INJECT_FDCL_DATA_IND
•	Added "PhysicalSlotInformationTlv" (17)
•	Added "EVENT_LTE_ML1_ASDIV_ENHANCED" (2899)
•	Added following packets' new versions
"LTE LL1 CSF SE TM9 Results" (0xB138) Version 141
"LTE LL1 CSF CSIRS Chest TM9" (0xB148) Version 141
"LTE LL1 PUCCH CSF" (0xB14D) Version 141
"LTE LL1 PUSCH CSF" (0xB14E) Version 141
•	Displays
•	Adding support for NBIOT RealTime RSRP Display
•	Added OneWeb P1 displays
•	New display for NBIOT RRC State change plot
•	New GNSS L2/L5 measurements display
•	Added rows for scell3 in table  for LTE ML1 Serving Cell Measurement rssi sinr display
•	Added 3 new automation interfaces API for HTML displays
•	GUI
•	Add check all/uncheck all to the match dialog.
•	NV
•	Added new EFS NV items 74041,74042
•	Added EFS NV Item 74044
•	Added New EFS NV Item 74045
•	Added New EFS NV Item 74046
•	Added new EFS NV items 74047, 74048
•	Added New EFS NV Items 74049-74050
•	Added New EFS NV Items 74051-74053
•	Bug Fixes:
•	Automation APIs
•	Linked automation API DipSwitchMask to work correctly
•	Fixed SearchForEvent.pl automation sample script
•	Added handling for NV read error response
•	Fix to allow SetSearchString() to search multiple keywords
•	Fix for GetItemSummary API
•	DBs
•	Fixed 0xB193 Filtered RSRP/RSRQ
•	Updated QMI_PDS_GNSS_MEASUREMENT_REPORT_IND message
•	Updated following 15 messages:
QMI_UIM_READ_TRANSPARENT (32)
QMI_UIM_GET_FILE_ATTRIBUTES (36)
QMI_UIM_DEPERSONALIZATION (41)
QMI_UIM_REFRESH_GET_LAST_EVENT (45)
QMI_UIM_GET_CARD_STATUS (47)
QMI_UIM_POWER_UP (49)
QMI_UIM_STATUS_CHANGE_IND (50)
QMI_UIM_REFRESH_IND(51)
QMI_UIM_GET_CONFIGURATION (58)
QMI_UIM_SEND_APDU (59)
QMI_UIM_GET_ATR (65)
QMI_UIM_PERSONALIZATION (76)
QMI_UIM_TEMPORARY_UNLOCK_STATUS_IND (95)
QMI_UIM_GET_PROFILE_INFO (100)
QMI_UIM_ADD_PROFILE (104)
•	Displays
•	Add start and end diag requests before sending pdapi commands in GNSS Fix Collection display
•	Formatting the copy to clipboard option with spacing and alignment
•	New GNSS RF Status Display for Version 5
•	Fix the font size for a table within a display
•	Item/Filtered Views
•	Fix for refiltering QSH Metric type
•	Disable hide/unhide columns feature in the command output window
•	NV
•	Updated EFS NV Item 67330
•	Updated EFS NV Item 67332
•	Updated EFS NV Item 70289
•	Updated EFS NV Item 73708
•	DMC Updates: 
•	Default DMC version unchanged at version 9
•	Resolved following JIRA tickets: 
JIRA	Title	Raised by	
QXDM-2675	[Automation API] QXDMDipSwitchMask.pl not work on QXDM4.0.182	QCT Applications Engineering SH	
QXDM-2882	QXDM4 Automation script: QXDMClientRequestNVID.pl & SearchForEvent.pl executed failed	QCT Applications Engineering SH	
QXDM-2953	API Support in QXDM for QSH	QCT Modem SW - LTE SD	
QXDM-3072	QXDM NV Read API issue with 70310	Internal	
QXDM-2510	Need information regarding QXDM API to get RX Rate	QCT QST CPT CPU SD	
QXDM-2956	[case:03146205][vivo]QXDM4,0194 SetSearchString() not support Perl engine	QCT Applications Engineering SH	
QXDM-2930	qxdm4 log packet GetItemSummary return empty result	QCT Modem SW - LTE SD	
QXDM-2980	Re: [case:03131106]GPS NMEA update query	QCT Product & Tools SW Analytics & Global Automation SD	
QXDM-2359	CASE# 02976390-I want to view NB-IOT Field TX/RX Performance at QXDM4	QCT WT Modem SW Applications Engineering KOR	
QXDM-3029	RE: (MSTFT-146) Column not aligned when copying from QXDM4 to text processor	QCT QST MST Commercialization SD	
QXDM-2830	[QXDM4]Only LOW_LEVEL item can be shown in the discovered items	QCT IoE Applications Engineering SZ	
QXDM-3053	GNSS RF Status window update in QXDM for Gen9VTv2	QCSR Location Tech - Bangalore	
QXDM-3013	Request to add new QXDM display - Pre5G RRC State Change Plot (FR 46355)	QCT QST MST Technologies SD	
QXDM-2823	font size for tables	Internal	
QXDM-2953	RE: API Support in QXDM for QSH	QCT Modem SW - LTE SD	
QXDM-3101	New GNSS L2/L5 measurements display needed	QCT Location Technology SCL	
QXDM-2985	Missing QXDM3.14 feature - Select all |Deselect All missing?	QCT Modem SW - LTE SD	
QXDM-3006	FR 46016: Add Scell3 to "LTE ML1 Serving Cell Measurements Display” and release data 11/17/17	QCT Software Target Program Management	
QXDM-2861	[QXDM4.00.186]Can't unhide(restore) the contents of command output after hide them	External	
QXDM-3138	case:03190132 Does AddSubsysV2ImmediateResponse and AddSubsysV2DelayedResponse available	External	

Latest QXDM Professional Software Version 04.00.00200 (10/20/2017).

•	New Features:
•	DBs
•	Added version 141 of "LTE LL1 Serving Cell RS" (0xB134) packet
•	Added version 32 of "LTE ML1 Intra Frequency Cell Reselection" (0xB181) packet
•	Added version 6 of "OW LL1 PDCCH Decoding Result" (0xB530) packet
•	Add following 2 AT messages:
QMI_AT_REG_AT_CMD_FWD_EX (37)
QMI_AT_FWD_AT_CMD_EX_IND (38) 
•	Added "IMS VDJ Dequeue" (0x15CC) V3
•	Added "LTE ML1 DLM BIMC Stats" (0xB1E3) Version 33
•	Added following 11 "GenLong" (0xB193) sub packets:
Sub packet 16 version 32
Sub packet 17 version 32
Sub packet 18 version 36
Sub packet 19 version 34
Sub packet 20 version 32
Sub packet 21 version 32
Sub packet 22 version 32
Sub packet 23 version 32
Sub packet 22 version 32
Sub packet 24 version 32
Sub packet 37 version 32
•	Added "Atuner Detune Info" (0x19ED) V0
•	Added "LTE LL1 Serving Cell CER" (0xB122) version 141
•	Added "LTE GM TX Report" (0xB16D) Version 9, "LTE UE Identification Message Report" (0xB169) Version 2
•	Added following 9 new QMI PDS messages:
QMI_PDS_SET_SPOOFING_REPORT_CONFIG (159)
QMI_PDS_GET_SPOOFING_REPORT_CONFIG (160)
QMI_PDS_SET_GNSS_ENGINE_MONITOR_REPORT_CONFIG (161)
QMI_PDS_GET_GNSS_ENGINE_MONITOR_REPORT_CONFIG (162)
QMI_PDS_SET_GNSS_REPORTING_CONFIG (163)
QMI_PDS_GET_GNSS_REPORTING_CONFIG (164)
QMI_PDS_EVENT_SV_INFORMATION_IND (165)
QMI_PDS_EVENT_GNSS_MEASUREMENT_USAGE_REPORT_IND (166)
QMI_PDS_EVENT_GNSS_TIME_CONV_PARAM_REPORT_IND (167)
•	Added "LTE ML1 System Scan Results" (0xB18E) Version 32
•	Added following packets
LTE PRACH Configuration (0xB166) Version 32
LTE Random Access Request (MSG1) Report (0xB167) Version 32
LTE UE Identification Message (MSG3) Report (0xB169) Version 32
LTE DCI Information Report (0xB16C) Version 35
LTE GM Tx Report (0xB16D) Version 34
•	Added "LTE ML1 CA Metrics Log Packet" (0xB184) Version 25
•	Added "TDSCDMA FW TS0 Midamble Detection Results" (0xD106) Version 141
•	Added 0x00013295 (DTMF) media type to vocoder packets 0x1804 / 0x1805 / 0x1914 / 0x1915
•	Added "LTE PDSCH Stat Indication" (0xB173) version 17
•	Added "LTE LL1 RS Signal Correlation" (0xB120) version 121
•	Added version 3 of 0x1959 QDR DR Raw Sensor Data and new bit decoding in flag2 for 0x1476
•	Added version 125 of "LTE LL1 PUSCH Tx Report" (0xB139). version 122 of "LTE LL1 RACH Tx Report" (0xB144)
•	Added "LTE ML1 eDRX SLEEP" (0xB1E0) version 17
•	Added version 3 of 0x1959 QDR DR Raw Sensor Data
•	Added "LTE RLC DL Config" (0xB081) version 2 and "LTE RLC DL AM All PDU"  (0xB081) version 4
•	Added new bit parsing for PosFlag2 of 0x1476
•	Added 5 new TLVs in  "QMI_PDS_SET_GNSS_MEASUREMENT_REPORT" message
•	Added parser for 0x19F8 - LOG_GNSS_ME_NAV_E911_CONCURRENCY_STATUC_C
•	Added following packets:
LTE UE Identification Message (MSG3) Report (0xB169) Version 40
LTE DCI Information Report (0xB16C) Version 40
LTE GM TX Report (0xB16D) Version 40
LTE ML1 GM ACH Tput Report (0xB1AC) Version 40
•	Added "LTE LL1 Rx Agc Log" (0xB111) version 122
•	Added "Task Priority" (0x1922) Version 2
•	Added "LTE PDSCH Stat Indication" (0xB173) Version 37
•	Added following 10 "LTE ML1 Serving Cell Meas Response" Subpacket ids:
Sub packet 16  version 40
Sub packet 17  version 40
Sub packet 18  version 40
Sub packet 19  version 40
Sub packet 20  version 40
Sub packet 21  version 40
Sub packet 22  version 40
Sub packet 23  version 40
Sub packet 24  version 40
Sub packet 37  version 40
•	Added "QMI Indication QMI_PDS_EVENT_GNSS_CLOCK_MODEL_INFORMATION_IND" (168) and upated QMI_PDS_GNSS_MEASUREMENT_REPORT_IND(145) and QMI_PDS_SET_GNSS_REPORTING_CONFIG_REQ (163) messages
•	Added "LTE ML1 BPLMN Cell Confirm" (0xB1A2) version 32
•	Added following GSM packets:
"GSM DSDS Antenna Switch Diversity" (0x5A8A) Version 1
"GSM DSDS DFT ACI Metric" (0x5A95) Version 1 and 2
"GSM DSDS L1 RX Diversity Metrics" (0x5A96) Version 1, 2, 3, 4, 5 and 6
"GSM DSDS Parallel SCH Metrics" (0x5A98) Version 1
"GSM DSDS L1 New SCH Acquisition Metrics" (0x5412) Version 1 and 2
"GSM DSDS L1 New FCCH Decode Metrics" (0x5413) Version 1
•	Added "LTE RLC UL Config" (0xB091) version 3 and "LTE RLC UL AM All PDU"  (0xB092) version 4
•	Displays
•	Added new display PMIC ADC to read the ADC and TSENS channel's data
•	Support to show the packets registered with each display
•	Add 3 new displays for the 5G demo
•	Added New OneWeb display OneWeb RRC State Change Plot
•	Added OneWeb display OneWeb ML1 FL Throughput and BLER
•	Adding support for NBIOT RealTime RSRP Display
•	GUI
•	Adding shortcut ctrl+shift+w for close all windows
•	NV
•	Added New EFS NV Item 74025
•	Added New EFS NV Item 74026
•	Added EFS NV Items 74027,74028
•	Added new EFS NV Item 74029
•	Added EFS NV Items 74030,74031
•	Added new EFS NV item 74032
•	Added New EFS NV Item 74033
•	Added New EFS NV Items 74034,74035
•	Added EFS NV Item 74036
•	Added new EFS NV item 74037
•	Added new EFS NV Items 74038,74039
•	Added New EFS NV Items 74040,74041
•	Parsing
•	Added Qcat/Apex COM parsing support
•	Added the parsing support for "LTE RRC OTA Packet" (0xB0C0) V20, LteRrcVE30
•	Added QCAT/APEX com parsing for 0x1098
•	Other
•	Implemented third party device detection
•	Feature support for Multi Sim UI currently for Filtered Views, Graphs and HtmlViews
•	Bug Fixes:
•	Automation APIs
•	Fix for issue with closing item store in automation
•	Fix for F3 decoding issue.
•	Added the flag to include full parsed text in the data exported to file
•	Fixes for SetSearchString automation API
•	Resets packet ID when device disconnects
•	Fix for return type of GetFieldValue automation API
•	Fix for bug in SearchForEventOccurrences
•	GetFieldValue returns an appropriate value for UInt64 values
•	Fixed an issue with automation API SetQShrink4ServerPath
•	Implement SetLoggingOn/SetLoggingOff functionality in a perl module
•	Linked automation API DipSwitchMask to work correctly
•	DBs
•	Updated following 7 messages:
QMI_AT_RESET (0)
QMI_AT_REG_AT_CMD_FWD (32)
QMI_AT_FWD_AT_CMD_IND (33)
QMI_AT_FWD_RESP_AT_CMD (34)
QMI_AT_ABORT_AT_CMD_IND (35)
QMI_AT_SEND_AT_URC (36)
QMI_AT_DUMMY_AT_CMD_IND (255)
•	Fixed "GSM L1 G2X Tune Away" (0x50A4) "TA Abort Reason" enum
•	Fixed event 1968 and 1969 "NAS EMM OTA outgoing message ID" and "NAS EMM OTA incoming message ID" enum strings
•	Fix for issue with "Vendor Database Path" configuration
•	Fixed 0xB122 "Carrier Index"
•	Displays
•	Fix for GNSS Search Strategy Task Allocation display
•	Fix for LTE ML1 Serving Cell Measurements display
•	Adding support for Scell2/3/4 Info in LTE ML1 UL Throughput and BLER Display
•	Fix regression issue of false spikes while plotting empty point
•	GPS
•	Fix for QXDM failing to detect GPS devices
•	Properly register XGPS during QXDM installation
•	GUI
•	Fixed max/minimize button in filtered view when items matched/filtered
•	Item View / Filter View
•	Fix for Sync to Item functionality
•	Fix for Configure with Registration functionality
•	Fix for bug with item match
•	Remove Ctrl +C  option and add Ctrl+A for hexview ,itemview and property view
•	Fix for bookmark functionality in Message View and Log View
•	Fix for highlight functionality
•	Fix for inverted search functionality
•	Fix for timestamp changing when clicked
•	Fix the progress dialog x of total where x was incorrect.  Also, fixed search criteria persistance
•	Fixed issue that dup annoation added when choosing any annotation items.
•	Implemented QXDM3 Command APIs "logging on", "logging off", and "set_log_dir"
•	Resolved several issues with discovered items
•	NV
•	NV write automation changes to include EFS Sync
•	Updated EFS NV Item 69744
•	Edited EFS NV Item 73852
•	Updated EFS NV Items 73852, 73842, 73844
•	Updated EFS NV Items 72594,73709
•	Edited EFS NV Item 67331
•	Updated EFS NV Item 73763
•	Updated EFS NV Items 73842,67330
•	Packaging
•	Fix packaging of rrc libs in windows build
•	Parsing
•	Fixed  "WCDMA Signaling Messages" (0x412f), channel 240
•	SILK
•	Updated the 'protocol configuration' IE to release 14
•	Other
•	Changed table properties to non editable
•	Changed the text when PNG file not installed
•	Windows Title [Logging] update fixes
•	Treat an integer string as a hex value in a set password diag command
•	Fix for stability issue during ISF to DLF conversion
•	DMC Updates: 
•	Default DMC version unchanged at version 9
•	Resolved following JIRA tickets: 
JIRA	Title	Raised by	
QXDM-2757	No GPS on QXDM	CORPORATE ENGINEERING	
QXDM-2781	QXDM4.00.186 Version Does Not Detect GPS Device	QCT IoE Applications Engineering SZ	
QXDM-2717	Add the third party device auto detect in QXDM4	External	
QXDM-2148	How to close single log with perl in QXDM4?	QCT Applications Engineering SH	
QXDM-2890	QXDM4 Logging issue	QCT Modem SW - I&T SD	
QXDM-2886	NV write via APS Fails	Internal	
QXDM-2843	Perl script to write NV items in QXDM4	Internal	
QXDM-2683	Issue while exporting text using automation	QCT Location Tech-Hyderabad	
QXDM-2252	QXDM4: GetClientItemCount interface	QCT Location Technology SCL	
QXDM-2816	NV is read as 0 even thought it is shown as 1	Internal	
MPSSMTF-9264	WrieteNV failing with QXDM	Internal	
QXDM-2667	QXDM4 can't parse 0x4023(WCDMA Uplink and downlink power) log	Internal	
QXDM-2585	QXDM4 couldn't parse 0x1098 RUIM debug	Internal	
QXDM-2820	Syncing to item not working!	QCT Modem SW - LTE SD	
QXDM-2800	Configure with Registration shows wrong data	QCT Applications Engineering TWN	
QXDM-2836	QXDM4.0 "Build information"window can't be editable issue	QCT Applications Engineering SZ	
QXDM-2854	No items matched on QXDM4	QCT Modem SW - IMS SD	
QXDM-2583	[case:03031443][<CUSTOMER>]QXDM4 can't use "Atrl C" "Ctrl A" etc. in parse window	QCT Applications Engineering SH	
QXDM-2832	Search Strategy Window Not populated	QCT Location Technology SCL	
QXDM-2873	RSRP of invalid Rx is displayed as "0" in LTE ML1 Meas window	QCT QST MST Commercialization SD	
QXDM-2869	"Logging" label does not work	Internal	
QXDM-2647	QXDM4 Inverted Search doesn't work	Internal	
QXDM-2847	PC timestamp always changes when click on it	Internal	
QXDM-1871	RE: User HTML display does not create separate MSIM displays	QCT QST MST Technologies SD	
QXDM-2059	How to add dashboard to QXDM to read ADC & TSENS	QCT Core Technologies Wired Connectivity SW SD	
QXDM-2474	Determining which log packets are used for any QXDM display	Nomad SIT Eng	
QXDM-2863	0x1098 parsing issue	Internal	
QXDM-2915	QXDM4: Options Menu Not Working	QCT IoE Applications Engineering SZ	
QXDM-2945	QXDM SearchForEventOccurrences API : not considering Search String	QCT Modem SW - 5G Air Interfaces BLDR	
QXDM-2962	WriteNV failing with engineering QXDM version 4.00.195.05	Internal	
QXDM-2937	Adding shortcut ctrl+shift+w for close all windows	QCT Modem SW - LTE SD	
QXDM-2939	[case:03140369][<customer>]Search/Re-filter windows no "max/min/close" button	QCT Applications Engineering SH	
QXDM-2650	QShrink/RUMI question	Internal	
QXDM-2970	WCDMA RRC OTA Messages are decoded on Win10 machine, on Win7 it is working	QCT QST MST Commercialization GRMNY	
QXDM-2874	LTE ML1 UL Throughput and BLER	QCT Applications Engineering TWN	
QXDM:2990	Search Type and Content is not being persisted	Internal	
QXDM-2994	Progress Dialog shows incorrect value for x in x of total	Internal	
QXDM-2999	Requesting to add Paint option in QXDM	Internal	
QXDM-2969	QXDM4: false spikes in WCDMA Power (Tx and sec Rx	QCT QST MST Commercialization ASTR	
QXDM-3008	QXDM 4.0 could not decrypt UE with Password by command while v3.14 is ok	External	
QXDM-2675	[Automation API] QXDMDipSwitchMask.pl not work on QXDM4.0.182	QCT Applications Engineering SH	
QXDM-2359	CASE# 02976390-I want to view NB-IOT Field TX/RX Performance at QXDM4	QCT WT Modem SW Applications Engineering KOR	
QXDM-2830	[QXDM4]Only LOW_LEVEL item can be shown in the discovered items	QCT IoE Applications Engineering SZ	

Latest QXDM Professional Software Version 04.00.00194 (9/15/2017).

•	New Features: None
•	Bug Fixes:
•	Fixed the return value of getFieldValue automation API for boolean values
•	Fix for F3 decoding issue.
•	DMC Updates: 
•	Default DMC version unchanged at version 9
•	Resolved following JIRA tickets: 
JIRA	Title	Raised by	
MPSSMTF-9144	RE: WriteThinUINvItem failure - QXDM 4.0.191	QCT Modem SW - I&T SD	
QXDM-2890	QXDM4 Logging issue	QCT Modem SW - I&T SD	

Latest QXDM Professional Software Version 04.00.00188 (8/18/2017).

•	New Features:
•	Enhancement for data aggregation between QXDM and QPST
•	SILK upgraded to Rel 13
•	Added following IEs:
DCI ID
SMS Service Status
Extended EMM cause
Hash MIME
Replayed NAS message container
•	Updated following messages:
Attach Accept message
Attach Reject message
Control SERVICE Accept message
GUTI REALLOCATION COMMAND message
Security Mode command message
SECURITY MODE COMPLETE message
TRACKING AREA UPDATE ACCEPT message
TRACKING AREA UPDATE REJECT message
•	Added version 5 of "WWCoex Power Info" (0x17F7) packet
•	Implemented NBIOT Uplink Tx Display
•	Added version 33 of "LTE ML1 PMCH Decode Results" (0xB1BC) packet
•	Add new feature message post-repairing processing
•	Add following 10 new versions:
0xB282	V2X FW Demfront PSCCH/PSSCH [Version 2]
0xB283	V2X FW Time Domain Channel Impulse Response [Version 2]
0xB284	V2X FW Whitened Matrices [Version 2]
0xB285	V2X FW PSCCH Decoding [Version 2]
0xB286	V2X FW PSSCH Decoding [Version 2]
0xB287	V2X FW Demfront MK Results [Version 2]
0xB288	V2X FW PSSCH Time Domain Channel Impulse Response [Version 2]
0xB28A	V2X FW Tx ACG [Version 2]
0xB28B	V2X FW Tx PSSCH [Version 2]
0xB28C	V2X FW Tx PSCCH [Version 2]
•	Added Version 3 of "iWLAN_S2B_IKEv2 ", 0x194F packet
•	Added EFS NV items 74018,74019
•	Added EFS NV Items 74020-74022
•	Added version 121 of "LTE LL1 UERS SNR" (0xB14F) packet.
•	Added EVS vocoder bandwidth information to Vocoder Statistics display
•	Added New EFS NV Items 74022,74023
•	Added Version 1 of "RF MAAT Internal Data" (0x19B5)  and version 121 of "LTE LL1 Neighbor Cell Measurements and Tracking" (0xB119) packet
•	Added version 127 of "LTE LL1 CSF Adaptation" (0xB147) packet
•	Added version 2 of 0xB091  "LTE RLC UL Config Log packet" sub packet 69.
•	Added UIM ISIM App Support
•	Added "LTE ML1 Profile Activity" (0xB1EC) packet
•	CDMA Retrievable Parameter display added
•	Added "GSM DSDS Log IQ" (0x5AA7) and version 27 of "LTE ML1 Multisim Packet" (0xB182) packets
•	Add 0x9407 (CSI Rx Report) header_version v1/v2 - packet_version v2
•	Added "LTE_PDCP_LOG_SUB_ID_UL_STATS" (0xB0B4) Sub packet: 0xC5  version 26
•	Added version 3 of "LTE NB1 FW DBack NPDSCH Asg" (0xB216) and "LTE NB1 FW DBack NPDSCH Decode Result" (0xB228) packets
•	Added version 125 of "LTE LL1 Rx On Toggle Info" (0xB136) packet
•	Added "OW LL1 SRS Tx Report" (0xB540) packet
•	Added following packets
V2X FW Time Domain Channel Impulse Response (0xB282) Version 3
V2X FW Whitened Matrices (0xB284) Version 3
V2X FW Demfront MK Results (0xB287) Version 3
V2X FW PSSCH Time Domain Channel Impulse Response (0xB288) Version 3
•	Added "MCPM General Session Power" (0x1874) packet V2
•	Added Rank3 and Rank4 CQI plots for all carriers (PCC, SCC1, SCC2, SCC3, SCC4)
•	Add 0x423E (EWC Debug Info) v12
•	Added version 2 of 0x1966 QDR GNSS SV State Data
•	Added version 3 of "V2X FW PSCCH Decoding" (0xB285) packet
•	Added version 2 of 0x1966 QDR GNSS SV State Data
•	Added the synthetic fields PWR and SNR
•	Added Version 3 of "MCPM General Session Power" 0x1874 packet
•	Added version 34 of "LTE ML1 PMCH Decode Results" (0xB1BC) packet
•	Added "OW PDCP DL Control PDU" (0xB4A2) and "OW PDCP DL Control PDU" (0xB4B2) packets
•	Added version 43 of "LTE LL1 PCFICH Decoding Results" (0xB12A) packet
•	Added event "EVENT_QSH_EVENT_TRIGGERED" (2885)
•	Added version 32 of "LTE ML1 Measuring Cell Result" 0xB196
•	Added following 5 new DMS messages:
QMI_DMS_INDICATION_REGISTER (3)
QMI_DMS_SET_DEVICE_CAP_CONFIG (101)
QMI_DMS_PSM_SET_CFG_PARAMS (102)
QMI_DMS_PSM_CFG_PARAMS_CHANGE_IND (103)
QMI_DMS_IMS_CAPABILITY_IND (104)
•	Added New EFS NV Item 74024
•	Added version 4 of "V2X FW PSCCH Decoding" (0xB245) packet
•	Added new display "NBIOT Serving Cell Measurements RSSISINR"
•	Bug Fixes:
•	Implemented SetScriptPath command
•	Fixes for stability issues in automation
•	Enhancements to guarantee windows can't get "lost" off the edges of the screen
•	Fixes to correctly populate HDR Air Link Summary window
•	Added new ONE-WEB Ext servide (99) and 30 new messages
•	Fixed the LTE ML1 PMCH Throughput BLER display to handle version 32 and added robustness in case of a corrupt log
•	Fix for issue where WCDMA OTA 0x412F with multisim header wrongly marked as malformed
•	Fix for LTE ML1 Serving Cell Measurements RSSI SINR display issues with SINR
•	Fixes for stability issues when loading DMC
•	Fix for QXDM to properly handle multisim headers
•	Fixes for issues with window titles
•	Fix for auto-connect to last device functionality
•	Fix for ADPL MUX ID
•	Fixes for text height issues in Item View and Filtered View
•	Fixes for WCDMA Power display
•	Fixed error for EFS NV item 70253
•	Bookmark view highlight color change
•	Made config item names consistent
•	Correct precision,scale in xml file and migrate lte pdcp throughput graph to qplot
•	Changes to improve perfomrance in GNSS Position Report
•	Power SAR display Update per 0x194E packet change
•	Updated to display NA if RSRP/RSRQ are 0 in linear scale or -30 dBm in log packet 0xB196
•	Fix for OTA 0x1086 Parsing Issue
•	Fixes for HDR Pilot Sets view
•	
•	Updated following 5 existing messages based on DMS spec 80-NH952-4 AD:
QMI_DMS_SET_EVENT_REPORT (1)
QMI_DMS_GET_DEVICE_CAP (32)
QMI_DMS_MODEM_ACTIVITY_INFO (95)
QMI_DMS_PSM_GET_CFG_PARAMS (96)
QMI_DMS_PSM_STATUS (98)
•	Updated EFS NV Item 71764, 73912
•	DMC Updates: 
•	Default DMC version unchanged at version 9
•	Resolved following JIRA tickets: 
JIRA	Title	Raised by	
QXDM-2495	RE: LoadDMCFile: Unable to connect to port 12	QCT Worldwide Eng Systems for Test SD	
QXDM-2750	QPST server crash is observed during log collection	QCT QST MST Technologies SD	
QXDM-2529	QXDM4 BUG (CRATFT) - HDR Air Link Summary window not populating	QCT QST MST Commercialization SD	
QXDM-2359	CASE# 02976390-I want to view NB-IOT Field TX/RX Performance at QXDM4.	QCT WT Modem SW Applications Engineering KOR	
QXDM-2651	QXDM4 - Version 4.00.185 - Frequent crashes seen	QCT QST MST Technologies SD	
QXDM-2626	QXDM filter out OTA log (0x412F) issue	External	
QXDM-2677	QXDM4 BUG LTE ML1 Serving Measurement Window Not Populating SINR value with LG G4 Commercial Device	Internal	
QXDM-2690	QXDM4 takes long time to launch with dmc	Internal	
QXDM-2679	QXDM4 not hanlding multisim header properly	Internal	
QXDM-2540	Serveral issues on QXDM 4 183	Internal	
QXDM-2692	RE: ADPL debug session	Data Service Team	
QXDM-2685	WCDMA Power window not getting populated broken in latest QXDM4 (FT-160)	QCT QST MST Commercialization GRMNY	
QXDM-2417	Displaying "EVS" vocoder bandwidth information in "vocoder statistics" view	QCT APTech Audio SW SD	
QXDM-2700	Modified NV 70253 failed	Internal	
QXDM-2304	FR 42564 Support for ISIM files in QXDM's UIM State Information Window	Internal	
QXDM-2452	Bookmark Lines difficult to Read	Internal	
QXDM-2482	QXDM4 ENH (CRATFT) - No CDMA retrievable parameters present	QCT QST MST Commercialization SD	
QXDM-2740	Config item name rule inconsistency	QCT Location Technology SCL	
QXDM-2668	RE: [case:03047508][03056631 ]QXDM4->View->LTE->RLC/PDCP TP issue	QCT Applications Engineering SH	
QXDM-2579	GNSS Position Report and Navigation DB display enhance request	QCT Location Technology SCL	
QXDM-2733	QXDM requirement from update of 0x194E	LTE team	
QXDM-2726	QXDM problems general and one specific	Nomad SW Eng	
QXDM-2744	Unable to parse HDR OTA in QXDM	Internal	
QXDM-2705	Data is not populating to HDR Pilot Sets view	QCT Applications Engineering SH	
QXDM-2661	Request for NB-IOT SNR and NRSSI plots	QCT QST MST Commercialization SD	

Latest QXDM Professional Software Version 04.00.00186 (7/25/2017).
•	New Features:
•	Implemented hide chart functionality
•	Added event 2880 "EVENT_LTE_TAM_MISS_TA_START_TIME"
•	Update Fusion CSM ans parser
•	Added version 24 of "LTE LL1 PDCCH Decoding Result" (0xB130) packet
•	Added "LTE ML1 Sleep Manager Summary" (0xB1EB) packet
•	Added function to convert from NV name to NV ID
•	Implemented QXDM QTrace %s static string support
•	Added version 124 of "LTE LL1 PUSCH Tx Report" (0xB139)
•	0x147B add bit masks parsing 
•	Added EFS NV Item 74007
•	Added Time Test Lite dialog
•	Added following 6 new NR5G ML1 packets:
0xB953 NR5G ML1 DL Cell Stat Config Request [Version 1]
0xB954 NR5G ML1 DL Time Slam Request [Version 1]
0xB955 NR5G ML1 DL Channel Config Request [Version 1]
0xB956 NR5G ML1 DL PDCCH RNTI Change Request [Version 1]
0xB957 NR5G ML1 DL ePBCH Decode Request [Version 1]
0xB958 NR5G ML1 ULRM MAC Schedule Request [Version 1]
•	Added version 4 of "LTE NB1 ML1 Cell Resel" (0xB24C)
Added following SSID messages:
MSG_SSID_SNS_FRAMEWORK   122
MSG_SSID_SNS_PLATFORM    123
MSG_SSID_SNS_SENSOR_INT  124
MSG_SSID_SNS_SENSOR_EXT  125
•	Added EFS NV Item 74008
•	Add following 10 new V2X packets
0xB281	LTE V2X FW Rx AGC
0xB282	LTE V2X FW Demfront PSCCH/PSSCH
0xB283	LTE V2X FW TD CIR
0xB284	LTE V2X FW Whitened Matrices
0xB285	LTE V2X FW PSCCH Decoding
0xB286	LTE V2X FW PSSCH Decoding
0xB287	LTE V2X FW Demfront MK Results
0xB28A	LTE V2X FW Tx ACG
0xB28B	LTE V2X FW Tx PSSCH
0xB28C	LTE V2X FW Tx PSCCH
•	Added confirmation dialog when clicking "New Items"
•	Implemented functionality to filter messages by level
•	Added "NR5G RFE Main" (0x1C01) packet
•	Added the support of OneWebRrcV1D0
•	Added "EVENT_IPA_TS_REWRITE_READY_ACK" (2881) event
•	Added version 25 of "LTE LL1 MPDCCH Chest Demod" (0xB145) packet
•	Added "EVENT_DTF_HANDLER_TRIGGERED" (2882) event
•	Added EFS NV Items 74009-74011
•	Added version 1 of "LTE NB1 ML1 Search PBCH Decode" (0xB250) and version 3 of "LTE NB1 ML1 Serv Cell Meas Response" (0xB24D)
•	Adding QDSS Device detection to QXDM4  + updated Connection dialog.  Phase 1 without Automation support for MAV devices. Bin file with comprerssed data supported.
•	Added following packets' new versions: 
0xB113 "LTE LL1 PSS Results" Version 121
0xB115 "LTE LL1 SSS Results" Version 122
0xB12E "LTE LL1 PBCH Decoding Results" Version 121
•	Added following 4 new WDS messages based on WDS spec 80-NH952-5 AH:
QMI_WDS_SUBSEQUENT_DATA_TRANSFER_STATUS (213) 
QMI_WDS_MODEM_ASSISTED_KA_START (214)  
QMI_WDS_MODEM_ASSISTED_KA_STATUS_IND (215)  
QMI_WDS_MODEM_ASSISTED_KA_STOP (216)
•	Added "OW LL1 FAP UL TIMING" (0xB515) packet and updated "OW RLC UL Statistics" (0xB49B) packet
•	Updated Refiltering to reuse the shared pointer for configuration returned by Item Config Dialog.
•	Added version 0xB147 of "LTE LL1 CSF Adaptation" (0xB147) packet
•	Added "LTE V2X L1 Scheduler" (0xB2E0) and version 34 of "LTE ML1 QC ARD Status" (0xB1EA) packets
•	Added event "EVENT_VOICE_VOCODER_PROPERTIES" (Id 2883)
•	Added EFS NV item 74012
•	Updated following 12 WDS messages based on WDS spec 80-NH952-5 AH
QMI_WDS_START_NETWORK_INTERFACE (32)
QMI_WDS_GET_PKT_SRVC_STATUS_IND (34)
QMI_WDS_CREATE_PROFILE (39)
QMI_WDS_MODIFY_PROFILE_SETTINGS (40)
QMI_WDS_GET_PROFILE_SETTINGS (43)
QMI_WDS_GET_DEFAULT_SETTINGS (44)
QMI_WDS_GET_RUNTIME_SETTINGS (45)
QMI_WDS_DUN_CTRL_EVENT_REPORT_IND (99)
QMI_WDS_HANDOFF_INFORMATION_IND (155)
QMI_WDS_APN_PARAM_INFO_CHANGE_IND (185)
QMI_WDS_RESET_AND_MODIFY_PROFILE_SETTINgS (199)
QMI_WDS_SET_ATTACH_PROFILE_INFO (200)
•	Added event "EVENT_DS3G_TSRC_CHG" (2884)
•	Added "OW ML1 Paging DRX Request" (0xB57C) packet
•	Added logic to ensure that a Re-filtered View or Match-filtered view will have the same window size with its parent.
•	Added version 3 of "LTE NB1 ML1 GM DCI Info" (0xB244) and version 2 of "LTE NB1 ML1 GM TX Report" (0xB245)
•	Add version 4 of "LTE NB1 ML1 Serv Cell Meas Response" (0xB14D) packet
•	Add V3 of "LTE NB1 ML1 GM DCI Info" (0xB244) and V2 of "LTE NB1 ML1 GM TX Report" (0xB245) packets
•	Added EFS NV Items 74013,74014
•	Added "V2X L1 Pool Manager Grant Request" (0xB2E4) packet
•	Add Bandwidth info in the display "LTE ML1 Serving Cell Measurements"
•	Added support for WCDMA RRC Channel Type 240 
•	Added new TRM parser for new version support.
•	Added new packets:
(0x0B2C8) V2X_MAC_SPS_CONFIG
(0x0B2C9) LOG_V2X_MAC_DSTID_SUBSCRIBE
(0x0B2CA) LOG_V2X_MAC_TX_TB
(0x0B2CB) LOG_V2X_MAC_RX_TB
•	Add "NR5G MAC UL TB" (0xB880) packet
•	Added following 5 packets:
OW LL1 FW Message  (0xB510) (Version 1)
OW LL1 PDCCH Decoding Result (0xB530) (Version 5)
OW ML1 Scheduler Log (0xB5A7) (Version 1)
OW ML1 MCLT (0xB5AA) (Version 1)
OW ML1 Handover Timeline Info (0xB5D9) (Version 1)
•	Added EFS NV Items 74015, 74016
•	Added "V2X L1 Physical Channel Request" (0xB245) and "V2X L1 TX Packet" (0xB246) packets
•	Added "V2X L1 Pool Manager Grid Info" (0xB2E3) packet
•	Adding One web parsing library  OwRrcV1D0
•	Added Version 6 of "Data Modem IPA Stats" (0x184F) and  Version 3 of "IPA TCP ACK COAL Stats" (0x1962)
•	Added following packets
"OW GM TX Report" (0xB56D) Version 4
"LTE ML1 Modem Clocks" (0xB1DC) Version 1
"NR5G ML1 BMAD Stats" (0xB95A) Version 1
•	Added following V2X packets: "V2X L1 Synchronization Manager" (0xB2C1) and "V2X L1 DFN Timing" (0xB2C2)
•	Added version 102 of "LTE LL1 PUCCH CSF" (0xB14D) and "LTE LL1 PUSCH CSF" (0xB14E)
•	Added version 3 of "LTE NB1 Contention Resolution Message (MSG4) Report" (0xB243) and version 122 of "LTE LL1 VPE Scheduler" (0xB12B) packets.
•	Adding supporting for B0c0 version 17 and version 19.
•	Added the Lte Rrc Signaling packet V19 (0xB0C0, LteRrcVE22)
•	Added version 2 of "LTE NB1 FW UL TX Sched" (0xB218) and "LTE NB1 FW UL Time Tracking" (0xB21C) packets.
•	Added "V2X FW PSSCH Time Domain Channel Impulse Response" (0xB288) packet
•	Added New EFS NV Item 74017.
•	Added version 2 of "Call Manager Stats Event" (0x1991)
•	Bug Fixes:
•	Fixed implementation of CopyViewItems automation API
•	Add handles for string inputs that are the same as deliminator used in QXDM
•	Fixed logic to identify discovered items
•	Changed the profiling Stop command to work correctly
•	Fixed "LTE ML1 BPLMN Complete Indication" (0xB1A4) packet
•	Fixed GNSSFix Collection display to correctly show all events
•	Added code to automatically detect device connect and configure
•	Fixed [100/16384] "DS/IPA Accelerated DPL Request"
•	Edited EFS NV Item 67332
•	QXDM4 now instantiates it's own version of GPS Server
•	Ensure that the Command Window isn't too small.  Setup a minimum size.
•	Added correct RRC api to support WCDMA parsing , when LTE OTA has embedded wcdma ota log.
•	Fixed 0x1476 flag2 parsing
•	Removed markers from LTE ML1 Real Time RSRP display
•	Updated Bookmark item color to be consistent with QXDM3
•	Fixed NV operations through command to be case sensitive
•	Fix to display SCC2 in LTE ML1 Serving Cell Measurement Display
•	Fix for GetClientItem Automation API for multisim devices
•	Changes to show measurements status as Hex in GNSS Measurement window
•	Corrected EFS NV Item 71525 definition
•	Enhanced "LTE ARD Info vs. Time" with "LTE_ML1_QC_ARD_STATUS" (0xB1EA) packet
•	Support multiple call manager windows in QXDM4
•	Fix to populate CDMA Active Set Pilot Strength Window
•	Fix to knots -> mph conversion.
•	Fix for issue in CDMA Power Window where the cursor would disappear
•	Add DiagULog new components support
•	Fix for QXDM NV browser row heights overlaps
•	Added handling of QPST COM error
•	Fixes for COM APIs GetItemTimestampText, GetItemHWTimestampText, GetItemName, and GetItemSummary
•	Improved QXDM performance in high data rate scenarios
•	Fixed exceptions in QTrace error format messages
•	Fix to save/load settings from DMC
•	Enhancements in GNSS Position Report and Navigation DB display
•	Fixed "LTE ML1 Antenna Switch Diversity" (0xB1DA) RSRP data type & calculations.
•	Fixed RequestItem automation API
•	Fixed CopyViewItems automation API to correct export to isf instead of text
•	Edited EFS NV items 73912,73708,70248
•	Fix to properly display total dropped packets
•	Fix to keep selection in a filtered view after refiltering
•	DMC Updates: 
•	Default DMC updated to version 9
•	Resolved following JIRA tickets:
JIRA	Title	Raised by	
QXDM-1828	Radar 30516829 - QXDM4	QCT Applications Engineering - 01 SCL	
QXDM-2395	QxDM 4.0.181 - Issue in Automation API CopyviewItems()	QCT QST Linux APT SD	
QXDM-2468	NV Browser NV 67264 regManagerDiscoverSchedule issue	Internal	
QXDM-2492	<Customer>  NV 67264 could not write 5,5,5 to regManagerPDPFailureSchedule	Internal	
QXDM-2438	RE: [case:02971460][<Customer>] QXDM->Message Packet->discovered items differ from v3.14	QCT Applications Engineering SH	
QXDM-2214	Logging 0x1156 and 0x1157	QCT SW CE EngOps TWN	
QXDM-2496	Request to provide API to convert nv name to nv id.	QCT Worldwide Eng Systems for Test SD	
QXDM-2436	[case: 02980129][<Customer>]QXDM GPS GNSS Fix Collection Test Iterations	QCT Applications Engineering SH	
QXDM-2457	FR43770:QXDM QTrace %s static string support	Internal	
QXDM-2471	Unable to see "Time Test Lite" option in QXDM4	Internal	
QXDM-2323	TTL window not present in QXDM4	Internal	
QXDM-2435	[case:2974782][<Customer>]QXDM4 not support GPS device GlobalSat GPS BU-353-S4 Model USB	QCT Applications Engineering SH	
QXDM-2441	[case:02983038] QXDM4.0.180 "command output window" optimization	QCT Applications Engineering SH	
QXDM-2484	[case:03001219]QXDM4 not support WCDMA RRC message (version =13)	QCT Applications Engineering SH	
QXDM-2518	QXDM4 ENH (CRATFT) - add warning pop up dialogue box when selecting new items option in tool bar	QCT QST MST Commercialization SD	
QXDM-1958	[QXDM4]New feature - Add Refilter Items_By Level	QCT IoE Applications Engineering SZ	
QXDM-2442	[case:02988396][<Customer>]QXDM4 RSRP can frequently be very blurry	China CE	
QXDM-2037	Status for QXDM support for Diag over QDSS. 	QCT Core Technologies	
QXDM-2452	QXDM4 Bookmarked Lines difficult to read	Internal	
QXDM-1957	New feature - Add refilter configuration file save/load to avoid selecting the items repeated	QCT IoE Applications Engineering SZ  CE TEAM	
QXDM-2534	TDD-3DLCA (SCC-2 not displayed in LTE ML1 Serving Cell Measurement Display	QCT QST MST Technologies HYD	
QXDM-2503	GetClientItem returns different values under different scenarios.	QCT Worldwide Eng Systems for Test HYD	
QXDM-2565	Measurement Status wrong in GNSS measurement window	QCT Location Technology SCL	
QXDM-2569	EFSNV 71525 write/read issue with QXDM4.0.182	Internal	
QXDM-2085	Can not open multiple call managers at the same time on QXDM4	QCT QST MST Technologies SD	
QXDM-2530	QXDM4 BUG (CRATFT) - CDMA Active Set Pilot Strength window not populating	QCT QST MST Commercialization SD	
QXDM-2558	[case:03023636][<Customer>]QXDM4 GPS issue and block test, asking for v3.14 temp build?	QCT Applications Engineering SH	
QXDM-2481	QXDM4 BUG (CRATFT) - CDMA Power Window Cursor Disappears	QCT QST MST Commercialization SD	
QXDM-2597	DIAG Ulog Integration tool updates	Diag team	
QXDM-2478	Case 03010177 - CA display with CC bandwidth	Internal	
QXDM-2290	ASN decode for RRC SIB DB messages	Internal	
QXDM-2595	RE: PlusL|SDM660.LA.2.1|LWG+LWG|SR_SC| Invalid TRM Procedures	QCT QST MST Technologies HYD	
QXDM-2527	QXDM does not display the on all screen resolutions	External	
QXDM-2172	Fonts of NV browser are overlapped	External	
QXDM-2495	LoadDMCFile: Unable to connect to port 12 	QCT Worldwide Eng Systems for Test SD	
QXDM-2564	OW RRC OTA message support - OwRrcV1D0	CORP ENG - Corporate Product Test 	
QXDM-2563	Log saving issue	Internal	
QXDM-2549	Move certain QSetting to DMC per PdM and customers requested	Internal	
QXDM-2579	GNSS Position Report and Navigation DB display enhance request	QCT Location Technology SCL	
QXDM-2537	RE: LteRrcVC75 is added	Internal	
QXDM-2554	Re: QXDM installation issue	QCT Distribution Tools	
QXDM-2505	QxDM 183 - CopyViewItems API returns 0	QCT QST Linux APT SD	
QXDM-2550	Should the item dropped packet total display be populating in QXDM 4	QCT QST MST Commercialization SD	
QXDM-2499	QXDM4 ctrl+y would lost all sync up result	External	

Latest QXDM Professional Software Version 04.00.00182 (6/26/2017).
•	New Features:
•	Added EFS NV Items 73998-74000
•	Add version 124 of "LTE LL1 CSF Adaptation" (0xB147) packet
•	Added (SubId 4, Version 4) of 0xB17A LTE ML1 S Criteria Check Procedure
•	Added Version 3 of 0xB197 LTE ML1 Serving Cell Information
•	Added (SubId 11, Version 4) of 0xB191 LTE ML1 Intra Frequency Cell Reselection
•	Added 0xB532 OW LL1 PUSCH Tx Report Initial (Version 3), 0xB539 OW LL1 PUCCH Tx Report Initial (Version 1 & 2), 0xB53C OW LL1 PDSCH Decoding Results  (Version 1 & 2), 0xB544 OW LL1 RACH Tx Report Initial (Version 1)
•	Add "WLAN IP Header Info" (0x1A12) packet
•	Add version 26 of "LTE ML1 Multisim Packet" (0xB182) packet
•	Add "LTE LL1 Half CIR Status" (0xB15E) packet
•	Added QMI_WDS_DELETE_ALL_PROFILES (205), QMI_WDS_GET_LAST_3GPP_RAB_REJECT_INFO (206), QMI_WDS_3GPP_RAB_REJECT_IND (207), QMI_WDS_GET_THROTTLED_PDN_REJECT_TIMER_INFO(208), QMI_WDS_SET_THROTTLED_PDN_REJECT_TIMER_INFO(209), QMI_WDS_SET_EHRPD_FALLBACK_APN_LIST (210), QMI_WDS_GET_EHRPD_FALLBACK_APN_LIST (211), QMI_WDS_PDN_THROTTLE_INFO_IND (212)
•	Added MSG_SSID_QDR (119)
•	Added UIMDIAG_SIMLOCK_CK_LOCK_CMD Request/Immediate Response/Response
•	Add version 125 of "LTE LL1 CSF Adaptation" (0xB147) packet
•	Added version 34 of "LTE RRC CA Combos Debug" (0xB0CF) packet
•	Added [75/30] ADC/Version Request/Response, [75/31] ADC/Get Channel Info Request/Response, [75/35] ADC/Start Read Request/Response, [75/36] ADC/Get Readings Request/Response, [75/37] ADC/Recalibrate Request/Response
•	Add 0x9400 (PDSCH KPI Report) header_version v1/v2 - packet_version v2
•	Added version 33 of "LTE ML1 QC ARD Status" (0xB1EA) packet
•	Add 0x4344 (WCDMA Multi Carrier EUL Combined L1 MAC) v6
•	Add version 141 of "TDSCDMA FW Tracking Mode" (0xD100)
•	Bug Fixes:
•	Updated EFS NV Items 73851, 73848
•	Fixed bug with handling whitespace in a command request
•	Fixed the column widths in the table of MLOG Memory Profiling Display
•	Make colors more distinctive in LTE Video RTP Data Rate Packet Rate display
•	Fixes for search history to be available correctly in multiple filtered windows
•	Status representation is changed to hex from decimal for GPS/GLO
•	Fix so command output window will not gain focus due to automation commands
•	Changed color of RRC State/XO PMIC plots to make it look clear
•	Updated QMI_WDS_INDICATION_REGISTER (3), QMI_WDS_START_NETWORK_INTERFACE (32)
•	Fix for clearing property view and hex view
•	Fix for alt+d in re-filter view
•	Fix for QTrace interpretation issue
•	Fix to remove unnecessary "|" characters when saving a few as text
•	Fix for ISFSetSearchString automation API
•	Sending the correct command for configuring target to get OS profiling logs 0x1156/0x1157
•	Adding the complete list of MBIM CIDs provided by MST
•	Added new column for bandwidth information for evs codec info in VolTE status window
•	Fixed version 35 of "LTE ML1 Full Frequency Scan Results" (0xB175)
•	Fixed RegisterClient automation API
•	Fixed exception issue when calling CopyClientItems API
•	Enhancement to improve behavior upon delayed modem boot
•	DMC Updates: 
•	Default.dmc unchanged at version 8
•	Resolved following JIRA tickets:
JIRA	Title	Raised by	
QXDM-2382	FW: QXDM4.0.181 for internal users released	QCT QST Core Platform Test SD	
QXDM-2265	RE: MLOG memory viewer ported from QXDM 3.x to 4.x	QCT Modem Processor Subsystem Performance SD	
QXDM-2084	LTE Video RTP Data Rate Packet Rate window - save configuration doesn't work	QCT QST MST Technologies SD	
QXDM-2375	Re: QXDM4--Match items query..	QCT Product Organization Diagnostic Tools SD	
QXDM-2386	QXDM4 Measurement screen "stat" column format incorrect for GPS/GLO	Internal	
QXDM-2397	QXDM4 issue: Command Output Window keeps coming to focus	QCT Location Technology SCL	
QXDM-2379	[QXDM]04.00.176] - Color of LTE RRC State Change Plot	QCT IoE Applications Engineering SZ	
QXDM-2322	[case:02963720][Japan][<Customer>]QXDM4 "XO And PMIC Temperature"	QCT Applications Engineering SH	
QXDM-2335	Clear all doesn't clear IE's	QCT Modem SW - LTE HYD	
QXDM-2096	[<Customer>][case:02878038] bookmark alt+d not work for all bookmark items in re-filter view	QCT Applications Engineering SH	
QXDM-2407	QXDM 181 issue with QTrace message	QCT Modem SW - LTE SD	
QXDM-2144	Why is the saved text file corrupted?	QCT Modem SW - MMCP SD	
QXDM-2405	RE: APS/QXDM blocker issues which need attention	QCT Worldwide Eng Systems for Test SD	
QXDM-2430	[case:02984556][<Customer>][automation]2 issues for QXDMGetItem.pl	QCT Applications Engineering SH	
QXDM-2112	[Automation]ISFSetSearchString.pl not work while v3.14 is OK	QCT Applications Engineering SH	
QXDM-2294	[9x50/SDX20] -QXDM4 MBIM QBI message parsing issue	QCT QST MST Technologies SD	
QXDM-1964	RE: VoLTE Status window -- EVS codec and its bit-rate	QCT QST MST Commercialization GRMN	
QXDM-2403	RegisterClient does not work on latest QXDM4	QCT Location Technology SD	
QXDM-2479	CopyClientItems() method is causing QXDM4 to become unresponsive	QCT Architecture	
QXDM-2282	Updated: NV Read/Writes failure with QXDM4 177	QCT Modem SW - I&T SD	

Latest QXDM Professional Software Version 04.00.00180 (6/5/2017).

•	New Features:
•	LTE ML1 DL Throughput enhancement
•	Add support to parse Log packets for Nr 5G
•	Added version 35 of "LTE ML1 AdvRx IC Cell List" (0xB18F)
•	Added new EFS NV Item 73996
•	Add version 3 of "LTE NB1 ML1 Cell Resel" (0xB24C) packet
•	Add version 9 of "LTE DCI Information Report" (0xB16C)
•	Added EFS NV Item 73997
•	Add version 17 of "XO Frequency Estimation" (0x13D1) packet
•	Add 0x41AA (WCDMA DRX PICH Log Packet) v8
•	Implemented automation APIs SetSearchString and AddSearchContent
•	Add 92 ONE WEB Events
•	0x1476 Flag2 add new DGPSEngaged bit
•	0x1386/7 add special link_type 10 for QXDM Aggregated log
•	Added support for GPS LSM Report Segment Aggregation
•	Bug Fixes:
•	Removed extra logging when using AnnotateLog
•	Added the column setting in bookmark list view
•	Updated EFS NV Item 73995
•	Changes to deactivate QXDM during installation
•	Enabled "SNR RX0" and "SNR RX1" fields for "LTE LL1 USERS SNR" V22-V102 (0xB14F)
•	Enabled "SNR RX2" and "SNR RX3" fields for "LTE LL1 USERS SNR" V102 (0xB14F)
•	Edited EFS NV Item 73573
•	Made auto connection configurable
•	Bug fixes for QXDM command line handling for NV write operations
•	Fixed ADPL timestamp issue
•	Enhancement on handling empty string on creating diag buffer
•	Fix for GNSS GALL Measurements display
•	Enhancements for GNSS Position Report display
•	Fix for Modem-TenX port and OEM devices
•	Fix for GetXML() automation API
•	Fix for CGPS NMEA Control autoscroll performance issue
•	Fix for command interface to gracefully stop when QXDM is closed
•	Fixed CreateView automation API to return success when the view is already open
•	Fixed handling of extra whitespace in send_data requests
•	Added special handling on field names change to resolve qxdm3 and qxdm4 differences
•	DMC Updates: 
•	Default.dmc unchanged at version 8
•	Resolved following JIRA tickets:
JIRA	Title	Raised by	
QXDM-2213	Clarification for multiple prints in QXDM log while using APS command AnnotateLog	QCT QST MST Technologies SD	
QXDM-2205	column setting in bookmark list view cannot be memorized	QCT SW CE EngOps TWN	
QXDM-1431	QXDM - Request to enhance LTE plots "LTE ML1 DL Throughput and BLER" and "LTE ML1 Serving Measurements Display"	QCT QST MST Technologies SD	
QXDM-2196	Add 5G Rrc Decoding support in QXDM4	QCT Modem SW – 5G Air Interfaces SD	
QXDM-1976	Need to run QXDM -deactivate at the end of installer	Internal	
QXDM-2219	QXDM 4 connection	QCT Product Organization Target Stability Test SD	
QXDM-129	QXDM4 | No option LTE_Video_RTP_Data_Rate_Packet_rate_window	QCT QST MST Technologies SD	
QXDM-2300	"Conference uri" of NV 73842 is showing wrong value after updating through SCR command	QCT Product Organization Target Test Automation HYD	
QXDM-2285	RequestNVItemWrite doesn't write null string to NV	QCT SW CE EngOps TWN	
QXDM-2288	RE: 9x55 AT2.1 : FR 34865 - Incorrect time stamp in PCAP logs	QCT Modem SW - Data Services SD	
QXDM-192	[QXDM4] RequestNVItemWrite will write incomplete fields when quoted Fields has space inside	QCT QST MST Commercialization JPN	
QXDM-2307	QXDM4 GAL measurement show svState from DB	QCT Location Technology SCL	
QXDM-2226	GNSS Position Report window enhancement request	QCT Location Technology SCL	
QXDM-1707	Processing compressed data from <customer> PL, from QTF to QXDM4	QCT Core Technologies Platform Kernel Services SW SD	
QXDM-2329	RE: Question on customizing QXDM display	Internal	
QXDM-2296	[Customer][QXDM4-Automation]ISFGetXML.pl not work	QCT Applications Engineering SH	
QXDM-2099	Auto Scroll feature in CGPS NEMA Control doesn't work	QCT SW CE EngOps TWN	
QXDM-2207	[Automation] QXDM4 grep_isf.pl match function not work	QCT Applications Engineering SH	
QXDM-2337	QXDM Stop Working	CORP ENG - Corporate Product Test	
QXDM-2336	RE: QXDM 3 Tool License has been expired-->move to QXDM4	QCT QST Linux APT HYD	
QXDM-1916	FR41138:QXDM support GNSS OTA log session assembly & parsing	QCT Software APSS Tech Program Management	
QXDM-2382	FW: QXDM4.0.181 for internal users released	QCT QST Core Platform Test SDQXDM-2295	
QXDM-2295	[case:02952752][Huawei][QXDM4-automation] ISFGetFieldIndex.pl issue	QCT Applications Engineering SH	

Latest QXDM Professional Software Version 04.00.00176 (5/15/2017).

•	New Features: 
•	Add "SNS HLOS Request" (0x19D9) and "SNS HLOS Event" (0x19DA) packets
•	Add following packets new version: 0xB203 "LTE NB1 FW DRX Status" version 3; 0xB208 "LTE NB1 FW Search PSS Auto Corr Result" version 3; 0xB20A "LTE NB1 FW Search SSS Result" version 2; 0xB21A "LTE NB1 FW UL TX PUSCH" version 2; 0xB226 "LTE NB1 FW DBack NPDSCH Asg" version 2
•	Implemented logic to clean up old temporary ISF files
•	Added: 0xB950 "NR5G ML1 Manager Common Config"; 0xB951 "NR5G ML1 Manager Dedicated Config"; 0xB952 "NR5G ML1 Manager Handover"
•	Add NV Item 73989
•	Added logic for a new filtered view window to automatically keep the same visisble columns as the existing window
•	Add "LTE PDCP UL Discard RTP Data" (0xB0B7) packet
•	Add 0xB4C1 "OW RRC MIB Message" Packet
•	Add 0x9402 (PDSCH Tx Report) & 0x9403 (PHICH Tx Report) with header_version v1/v2 & packet_version v1 under "TBS -> LTE -> eNB"
•	Add "WLAN FW Channel Change" (0x1A0D) and "WLAN FW HW Mode Change" (0x1A0E)
•	Add version 2 of 0xB248 packet
•	Added EFS NV Items 73990,73991,73933
•	Add version 2 of "GPRS RLC Uplink Statistics" (0x5222) and "GPRS DSDS RLC Uplink Statistics" (0x5C22) packets
•	Added One Web Parsing suppoirt for 0xB4C0, 0xB4E2, 0xB4E3, 0xB4E5, 0xB4EC, 0xB4ED
•	"Okay" button added as a select and close option in connection dialog
•	Added support for ADPL files
•	The current DMC name is now displayed on the left side of the status bar
•	Added NV item 73992
•	Added ISF<-->DLF conversion in Tools menu
•	GPS status bar implemented
•	Add "LTE ML1 QC ARD Status" (0xB1EA) packet
•	Added MSG_SSID_DS_WLAN (5034)
•	Added support for special UMTS/GSM subscription ID events and logs without multi-sim headers
•	Add refilter configuration file save/load to avoid selecting the items repeated
•	Added new EFS NV Items 73994,73995
•	Implemented VerifySPC API in HelperFunctions4.pm
•	Add version 2 of "LTE NB1 ML1 Cell Resel" (0xB24C), "LTE NB1 ML1 Serv Cell Meas Response" (0xB24D) and "LTE NB1 NBR Cell Meas" (0xB24E) packets
•	Add version 123 of "LTE LL1 Macro Sleep" (0xB137) packet
•	Bug Fixes: 
•	Fixes for writing to NV 71527
•	Fix for GPS Latitude and GPS Longitude to appear correctly in status bar
•	Update NV Item 71527
•	Fix to properly display items in command output window during replaying logs
•	Fix for RegisterClient API issue
•	Fixed Automation code for CloseView
•	Fix to clear the ISF only when not in read mode and Log view is launched
•	Fix to ISFAddItem.pl automation sample, so that it will not close unrelated QXDM windows on exit
•	Fixed parsing of "GSM RR SACCH Measurement Report" (0x513A)
•	Fix for load dmc functionality
•	Added an interface to determine if the GPS Server com object has a device held open.  QXDM can then determine if the device is in use and can't be tested.  QXDM will list it as an available GPS device in that case.
•	Fixed regular expression matching on fully parsed text
•	Fix for Unhandled OTA Logs to be treated as regular logs packets
•	Edited NV 73564,73567,73540,73535,73990,72509,73763
•	Fix for "2G Neighboring Cell Information in GSM 2G/3G Serving And Neighbor Cell Information" display
•	Fixed bug with parsing of OTA log 0x513A
•	Fixed NV read/write issue for 73567
•	Optimized mass bookmarks in QXDM
•	Fix for GNSS Position Report display
•	Fixes for NV editing
•	Fixed a WCDMA RRC OTA name displaying issue with extra PSC and UARFCN in the headers
•	Removed payload from the ExportViewText output
•	Fixes for WCDMA RRC accumulator logic
•	Restart log view when device disconnected and re-connected, if the restart on disconnect flag is checked in Item StoreSettings
•	Updated "XO Frequency Estimation" (0x13D1)
•	Fix to clean up QXDM from registry during install and uninstall
•	Edit EFS NV Item 72537
•	Fix to correctly save and load a DMC crated by enabling Log Packets OTA
•	Fixed ISF File Size display in status bar
•	Fixed QXDM Nv browser display issues with hex number
•	Maintain Dynamic Status , Tree display state in between connection and disconnection
•	Stability fix when saving all logs as text
•	DMC Updates:
•	Default DMC updated to version 8
•	Newly added packets: 
Packet Type	Packet ID	Packet Name	
Log	0x4002 	WCDMA MAC UL Traffic Volume Measurement Report	
Log	0x4119 	WCDMA RLC UL States	
Log	0x411F 	WCDMA RLC DL States	
Log	0x4123 	WCDMA RACH Control Parameters	
Log	0x41C7 	WCDMA RLC UL TM	
Log	0x41C8 	WCDMA RLC UL UM	
Log	0x41C9 	WCDMA RLC DL TM	
Log	0x41CA 	WCDMA RLC DL UM	
Log	0x41CB 	WCDMA RLC UL AM	
Log	0x41CC 	WCDMA RLC DL AM	
Log	0x41CE 	MAC UL Cipher Configuration	
Log	0x4213 	MAC HS Reset	
Log	0x422A 	Watermarks Tracing Log Packet	
Log	0x4809 	WCDMA_RRC_LOG_AMR_CODEC_INFO	
MSG Packet	05503/01	Security/Internet Protocol Security/Medium	
MSG Packet	05503/02	Security/Internet Protocol Security/High	
MSG Packet	05503/03	Security/Internet Protocol Security/Error	
MSG Packet	05503/04	Security/Internet Protocol Security/Fatal	
MSG Packet	05503/05	Security/Internet Protocol Security/Debug	

•	Resolved following JIRA tickets: 
JIRA	Title	Raised by	
QXDM-2114	RE: NV Write not working appropriately resulting in TC failure	QCT Worldwide Eng Systems for Test SD	
QXDM-2147	QXDM temp folder safe to clear?	Client and Application Management	
QXDM-2164	<Customer> reported that the “GPS Latitude” and “GPS Longitude” on status bar is always 0	External	
QXDM-1746	QXDM4_Issue || SUB_ID/Payload/HW_Time_Stamp/ProcID/Tags are getting enabled by default in Filtered window	QCT QST MST HYD	
QXDM-2083	Re: No annotation in command output	QCT QST MST SD	
QXDM-2063	Issue for RegisterClient API	QCT SW CE EngOps TWN	
QXDM-2128	[EU_FT] [KPI Issue] KPI crash after it is stuck at "Phone 1 Connecting	QCT Worldwide Eng Systems for Test HYD	
QXDM-2125	[FT EU][QXDM4]Change request for QXDM4 in terms of ALT+L usage	QCT QST MST GRMNY	
QXDM-2148	How to close single log with perl in QXDM4?	QCT Applications Engineering SH	
QXDM-2195	OneWeb Packet.. QXDM Jira for OneWeb support	Corporate Product Test	
QXDM-2188	GPS can't be connected for 2 QXDM4 instances	QCT IoE Applications Engineering SZ	
QXDM-2192	match feature NOT work for regular expression	QCT Location Technology SCL	
QXDM-2182	Request for QXDM4 Enhancement for connect/disconnect devices	QCT QST MST Technologies SD 	
QXDM-1891	0x513A parsing issue	QCT SW CE EngOps TWN	
QXDM-2199	RE: Not able to read/write NV items on SDX20	QCT QST MST Technologies HYD	
QXDM-2027	QXDM4 crashes when bookmarking a large number of log packets at the same time	China C	
QXDM-2187	RE: MTF - "ConfigureIMSServerType('zte')" keyword NV write is fail and MO VoLTE call is failing	QCT QST MST Technologies HYD	
QXDM-2220	QXDM 175 issues with NV 73833	QCT Modem SW - Data Services SD	
QXDM-1969	MAv16- TH2.1 - RRC OTA messages in getting logged in QXDM filtered window	QCT QST MST Technologies HYD	
QXDM-2055	FW: Automation is adding payload to QXDM logs	QCA CNSS MCL WLAN System Test HYD	
QXDM-1969	MAv16- TH2.1 - RRC OTA messages in getting logged in QXDM filtered window	QCT QST MST Technologies HYD	
QXDM-2241	RE: <PRISM-URL> - Updating Sub ID as part of UMTS DSDS NAS FPLMN List	QCT QST MST Technologies SD	
QXDM-1957	[QXDM4]New feature - Add refilter configuration file save/load to avoid selecting the items repeated	N/A	
QXDM-2119	Restart log view upon disconnect	N/A	
QXDM-1789	Re: Silent Uninstallation for QXDM4	QCT Worldwide Eng Systems for Test HYD	
QXDM-2206	QXDM4 doesn’t load customer’s dmc file correctly	QCT SW CE EngOps TWN	
QXDM-2260	RE: Issues while using QXDM4 for NV write/read	QCT Location Technology SCL	
QXDM-1792	Need QXDM4 api for automation to verify ServiceProgrammingCode	QCT QST MST Technologies SD	
QXDM-2039	window close when UUT resets	IPS Hardware	
QXDM-2275	Updated: QXDM crashing while exporting/saving all logs as text file	Internal WLAN user	

Latest QXDM Professional Software Version 04.00.00174 (4/17/2017).
•	New Features:
•	RRLP ASN update
•	Added B496 v2 (OW RLC UL UM Data PDU ), B486 v2 (OW RLC UL UM Data PDU) , B4A5 (OW PDCP SRB Integrity Data PDU), B56D (OW GM TX Report) , B530 v4 (OW LL1 PDCCH Decode Result)
•	Added 0xB4EB (OW NAS EMM Security Protected Outgoing Msg)
•	Added 0xB534 (OW LL1 Serving Cell RS)
•	Add "NR5G ML1 DLM Common Config" (0xB940) and "NR5G ML1 DLM Dedicated Config" (0xB941) packets
•	Add version 2 of "MCS CFCM Command Info" (0x18A8) packet
•	Add feature to show GPS information from an external GPS adaptor
•	Add "LTE NB1 ML1 Cell Resel" (0xB24C) and "LTE NB1 ML1 Serv Cell Meas Response" (0xB24D) packets
•	Add "LTE MAC ELS UL MCE Trigger" (0xB06A Sub 16)  and "LTE MAC ELS UL Transport Block" (0xB16B Sub 17) packets
•	Add "LTE NB1 ML1 Cell Meas" (0xB24E) packet
•	Add version 2 of "MCS CFCM Monitor Info" packet
•	Status bar now shows the DMC file name
•	Add "NR5G RRC Serving Cell Info" (0xB823) packet
•	Add 0x9401 (Pusch_KPI_Report) & 0x9407 (Csi_Rx_Report) with header_version v1/v2 & packet_version v1 under "TBS -> LTE -> eNB"
•	Add version 121 of "LTE LL1 Joint Demod" (0xB150)
•	Added Diag-Ulog integration
•	Decode Subsystem Dispatch Version 2 Response Header fields in the Item View summary column
•	Apply item list font setting to the full parsing area
•	Add version 33 of "LTE ML1 Common DC Offset" (0xB1B2)
•	Add version 3 of "RFLM XPT IQ Processing Results" (0x1980) packet
•	Version 27 of "LTE LL1 PDSCH Demapper Configuration" (0xB126)
•	Add version 28 of "LTE LL1 PDSCH Demapper Configuration" (0xB126) and version 27 of "LTE LL1 PDSCH Decoding Results" (0xB132)
•	Add version 35 of "LTE PDSCH Stat Indication" (0xB173) packet
•	Add SSID configuration for Re-filter
•	Add version 121 of "LTE LL1 Serving Cell FTL Corr" (0xB142) packet
•	Add 0x41D7 (WCDMA X2W Step1 Search Results ) v2, 0x41D8 (WCDMA X2W NAS-TT Search Results ) v2, 0x41D9 (WCDMA X2W List Search Results) v2
•	Bug Fixes:
•	Fixes for GPS connections
•	Fix for unstoppable command window scrolling
•	Updated LTE ML1 Serving Cell Measurements Display and LTE ML1 Serving Cell RSSI SINR Display
•	Fix for parsing of RRC OTA log packets
•	Fix for GNSS Navigation Database display
•	Updated TRM dll for parsing issue not following ICD
•	Fixes for GNSS GAL Measurements and GNSS Beidou Measurements displays
•	Fix to start in the most recently accessed location when saving an ISF
•	Bug fixes for writing to NV 65633
•	Fix for bug in Vocoder Statistics display
•	Fixes to save QPlot settings
•	Enhance QXDM device conneciton for different case
•	Fixed parsing for [0xD0E3] TDSCDMA RRC Signaling Packet
•	Fixed NV reading failure due to device port switched from automation
•	Fix for Item Store File issue
•	Fix decoding of NAS and GSM RR messages
•	Fixed the B0c0 parsing issues with packet version 16 and Vd22 parsing dll. Updated the summary column data
•	Fixed the 0x7B3A parsing
•	Fix for NV73862 mask definition issue
•	Fixed the parsing for 0x5B2F
•	Fix for device to show correct device connection status in GUI after disconnecting through automation API
•	Fix to ensure databases are always installed under ProgramData (if possible)
•	Fixed bug for using user defined parsing dlls with multi-sim packets
•	DMC Updates:
•	Default.dmc updated to Version 7
•	0xB06A LTE MAC ELS UL MCE TRIGGER (added)
•	0xB06B LTE MAC ELS UL Transport Block (added)
•	0xB1DC LTE ML1 Modem Clocks (added)
•	Resolved following JIRA tickets:
JIRA	Title	Raised by	
QXDM-1817	Issue on QXDM after GPS connection	QCT QST MST SD	
QXDM-1935	GPS connection failures	CORPORATE ENGINEERING	
QXDM-1977	Commandline window won't stop refreshing	QCT Product Organization Target Stability Test SD	
QXDM-2024	RE: ELS: RRC OTA log packets broken in QXDM view	Internal	
QXDM-1989	GNSS view issue: Navigation Database and GPS measurement	QCT Location Technology SCL	
QXDM-2050	L+L| Issue with Client Mapping for 0x12E8	QCT QST MST SD	
QXDM-1993	Three more issues in GNSS BDS & GAL measurement view	QCT Location Technology SCL	
QXDM-1995	Reuse latest used location for saving logs	QCT Modem SW - UIM Technology SD	
QXDM-2033	Re: QXDM 4 Missing GPS Report for External GPS Adapter	QCT QST MST SD	
QXDM-2057	ISSUE NV65633	QCT QST MST SD	
QXDM-2054	RE: Vocoder Statistics view bug for AMRWB 23.85	QCT APTech Audio SW HYD	
QXDM-1974	Status bar to show DMC file name	Internal	
QXDM-1828	Radar 30516829 - QXDM4	External	
QXDM-1302	FR37438:Diag Buffer (Diag-ULog integration)	QCT Software APSS Tech Program Management	
QXDM-1351	Decode Subsystem Dispatch Version 2 Response Header fields	QCT APTech Sensors SW SCL	
QXDM-1912	font size of decoded info	External	
QXDM-1968	QXDM4 disconnection issue	QCT SW CE EngOps TWN	
QXDM-2021	Seeing NV issues on Fusion target- Device Removed	QCT Modem SW - I&T SD	
QXDM-1967	[QXDM4 new requirement] Add SSID configuration for Re-filter	QCT Applications Engineering SH	
QXDM-2007	[Oppo] [QXDM4.00.168]Need to upgrade for 0xD0E3 | TDSCDMA RRC Signaling Packet |	QCT IoE Applications Engineering SZ	
QXDM-2078	Modem EFS not ready with QPST 459	QCT Modem SW - I&T SD	
QXDM-2117	Created: Verizon - Item Store File issue	QCT SW CE EngOps TWN	
QXDM-2108	NAS and GSM RR messages can't decoded properly	QCT IoE Applications Engineering SZ	
QXDM-2024	ELS: RRC OTA log packets broken in QXDM view	QCT Product Organization Diagnostic Tools SD	
QXDM-2064	[case: 02879954] QXDM4.00.171 could not parse OTA log while QXDM3.14 is OK	QCT Applications Engineering SH	
QXDM-2071	No GSM RR Messages logged via Automation runs	QCT Product Organization Diagnostic Tools SD	
QXDM-1919	automation API call disconnect successfully, however on GUI still shows connect	QCT Product Organization Target Stability Test SD	
QXDM-2107	[QXDM4 automation]DisconnectFromComport not work, while v3.14 is OK	QCT Applications Engineering SH	
QXDM-2110	[QXDM04.00.170]show the black splash screen when the first start	External	
QXDM-2129	Parser DLL not work on QXDM4 for some ISF	QCT Applications Engineering SH	

Latest QXDM Professional Software Version 04.00.00170 (3/23/2017).
•	New Features:
•	Add 0x41DE (Search Set Movement) v1
•	Add version 123 of "LTE LL1 CSF Adaptation" (0xB147) packet
•	Redesigned the LTE ML1 Connected Mode Display
•	Add event "EVENT_LTE_RRC_CELL_INFO" (2879)
•	Add 0x4186 (WCDMA Temporal Analysis Edition 2) v12
•	Add version 122 of "LTE LL1 Macro Sleep" (0xB137)
•	Added version 4 of "Logging Requested QoS , Ver2" (0x135A)
•	Add version 1 of "1xEV Tune Away Info" (0x1184) packet
•	Add following 8 new IMSS messages: QMI_IMS_SETTINGS_SET_QIPCALL_EVS_CONFIG (147), QMI_IMS_SETTINGS_GET_QIPCALL_EVS_CONFIG (148), QMI_IMS_SETTINGS_QIPCALL_EVS_CONFIG (149), QMI_IMS_SETTINGS_SEND_RTT (150), QMI_IMS_SETTINGS_RTT_RCVD_DATA (151), QMI_IMS_SET_BIND_SUBSCRIPTION (152), QMI_IMS_ACTIVE_SUBSCRIPTION (153), QMI_IMS_GET_ACTIVE_SUBSCRIPTION_STATUS (154)
•	Add version 123 of "LTE LL1 CSF Adaptation" (0xB147) packet
•	Add version 1 of "ATuner Internal Data" (0x18C4) packet
•	Enhancements for "QXDM status Dynamic window"
•	Bug Fixes:
•	Fix to correctly inherit column states in a refiltered view
•	Fix to generate the correct Sub ID when only SUB0 is active
•	Parsing enhancement for 0x1479
•	Add the data processing logic for 0xB193 version1 subversion 35 in display LTE ML1 Connected Mode RSRP RSRQ SNR
•	Added support for UARFCN and PSC data in 0x412F WCDMA RCC
•	Add UIM PDU parsing information into Summary column in QXDM for UIM APDU packet (0x19B7)
•	Fixes for Navigation Database and GPS measurement displays
•	Fix to properly open QXDM and load an ISF when the ISF has a Unicode filename
•	Make the item in configuration view not editable, and double click to open the category
•	Fix for QXDM to properly write NV 4703
•	Fix for QXDM to properly read NV 1206
•	Fix for NV Browser to properly display the value of NV 441
•	Fix to allow NV 1896 and NV 70310 to be properly set from QXDM
•	Fix to properly read NV 67218
•	Fix to properly write NV 69750
•	Fix to properly write band_pref_16_31
•	Resolved following JIRA tickets:
JIRA	Title	Raised by	
QXDM-1953	Some log packets and F3s have SUBID255 when only SUB0 is active	QCT Applications Engineering SH & TWN	
QXDM-1937	QXDM4 Cursor Couldn't update Legend Names	External	
QXDM-1971	MAv16- TH2.1 - RRC OTA messages is not getting logged in QXDM filtered window	QCT QST MST HYD	
QXDM-1989	GNSS view issue: Navigation Database and GPS measurement	QCT Location Technology SCL	
QXDM-1955	[QXDM4]ISF file can't open by double click if include Chinese character name or directory	QCT IoE Applications Engineering SZ	
QXDM-1816	QXDM real-time stat for NB1 Demo	QCT Modem SW - LTE SD	
QXDM-1949	Wingtech QXDM4.00.168, "re-filter config" issue	QCT Applications Engineering SH 	
QXDM-1566	RE: surface 2017 Case --> Our internal AIs	QCT Location Technology SCL	
QXDM-1702	RE: Case 02778147 - NV 01206 and similar not readable in qxdm4..works fine in qxdm3	QCT WT TAMs Applications Engineering SD	
QXDM-1900	QXDM4->NV browser, could input manually and but could not display correctly	QCT Applications Engineering SH	
QXDM-1889	QXDM4 Issue: NVs 1896 and 70310 can not be set to true	QCT QST MST SD	
QXDM-1859	Getting Bad EFS Respond error on QXDM4	QCT Product Organization Target Product SW I&T HYD	
QXDM-1819	NV Write Issue through RequestNVItemWrite commad	QCT Product Organization Target Test Automation HYD	
QXDM-1930	requestNVItemwrite command in QXDM4.0.165	QCT QST Linux APT SD	

Latest QXDM Professional Software Version 04.00.00168 (3/9/2017).

•	New Features:
•	Add version 122 of "LTE LL1 CSF Adaptation" packet
•	Bug Fixes:
•	Fix for autoscroll indicator
•	Fix for garbled strings and unresponsiveness in "CGPS NMEA Control" view
•	Fix to properly display "GNGNS" in "CGPS NMEA Control" view
•	Resolved following JIRA tickets:
JIRA	Title	Raised by	
QXDM-1931	QXDM crashes while replaying isf file with	QCT SW CE EngOps TWN	
QXDM-1759	"CGPS NMEA Control" window in QXDM not show GNGNS	QCT Location Technology SCL	

Latest QXDM Professional Software Version 04.00.00166 (3/8/2017).
•	New Features: None
•	Bug Fixes: 
•	Fix for NV Read on multi-sim
•	Fixed an exception issue related with F3 message processing
•	Resolved following JIRA tickets:
JIRA	Title	Raised by	
QXDM-1918	QXDM165: Consistent APS NV Read issue with EFS NVs	QCT Modem SW - I&T SD	
QXDM-1920	QXDM 165 crash	QCT Worldwide Eng Systems for Test SD	

Latest QXDM Professional Software Version 04.00.00164 (3/7/2017).
•	New Features: 
•	Add 16 new DSD messages
•	Add 3 new sub packets version into ML1 Sub packets (0xB193)
•	Add "LTE NB1 ML1 CDRX Events Info" (0xB248) packet
•	Updated "QMI_PDS_EXT_SV_IN_FIX_WITH_HEALTH_REPT" message based on PDS EXT spec 80-NH952-14 AD
•	Added functionality to change item colors
•	Updates to default DMC and CFGs
•	Add version 123 of "LTE LL1 PUSCH Tx Report" (0xB139)
•	Add version 34 of "LTE ML1 AdvRx IC Cell List" (0xB18F)
•	Added CAT-M1 and NB logmasks as secondary DMCs
•	Added "copy selected item" functionality to NV Browser
•	Add versoin 5 of "HDR SRCH RF TxD Event" (0x12BA) packet
•	Change to prefer Gps.db over Diag.db in GNSS views
•	Added Dynamic Item View to QXDM4
•	Added 0x147B v11 into "GNSS Navigation Database"
•	Add many ONE WEB packets and sub packets
•	Add version 129 of "LTE LL1 Serving Cell RS" (0xB134) packet
•	Create new IClientConfig APIs to RemoveLog, RemoveEvent and RemoveMessage
•	Adding v126 of B132 "LTE LL1 PDSCH Decoding Result" packet
•	Enhancement to display Debug Messages in Line# Filename and Debug message
•	Add 0x19D3 (ADSP USB In Out PCM Log) v1
•	Add version 16 of "LTE PLMN Search Request" (0xB0C3) packet
•	Bug Fixes: 
•	Fix for XO And PMIC Temperature display
•	Fixes for getValueTextWithFieldAccessPosString automation API
•	Fixes for GNSS Position Report display
•	Fixed automation issue in getEventName for new events like 2868
•	Fixed "EPS Network Feature Supported" IE
•	Fix for scrollbar issue when maximizing a filtered view
•	Fixed "QMI_VOICE_SET_CONFIG" -> UiTtyConfigStatusTlv
•	Fixes for Vocoder Statistics view
•	Fixed the parsing for CDMA 0x1004 log
•	Fixed issue with  Serving Cell Measurements display
•	Fixes for GNSS Navigation Database view
•	Fixes for arrow-key navigation of item view
•	Alpaca COM port fix
•	Fix displays flickering issue (gap in the lines) when item store preparing to do auto-save
•	Fix to allow columns to be unhidden after relaunching QXDM
•	Fix to keep the payload hidden after a refilter or match operation
•	Resolved following JIRA tickets:
JIRA	Title	Raised by	
QXDM-1727	XO And PMIC Temperature doesn't behave correctly	QCT SW CE EngOps TWN	
QXDM-1809	[QXDM4]can't change specific key item color on QXDM 4.X version	QCT IoE Applications Engineering SZ	
QXDM-1845	NV453 NV read issue with QXDM4.0.159 and 161	QCT Modem SW - I&T SD	
MPSSMTF-7535	SDM 660 || MTF is not catching WCDMA to LTE reselection events - WaitForEvent() = APS.1: Unknown Event ID =	QCT QST MST HYD 	
QXDM-1011	[QXDM4] Scroll bar transports to the first element in filter view when the filter view window is maximized {Auto Scroll Off]	QCT QST MST SD	
QXDM-1887	[Internal]QXDM4->NV Browser->right click function	QCT Applications Engineering SH	
QXDM-1842	EAMR and G711 Alaw tables not getting updated in vocoder statistics view - QXDM4	QCT APTech Audio SW HYD	
QXDM-1808	[VIVO]QXDM4 could not parse OTA log 0x1004, while v3.14 ok	QCT Applications Engineering SH	
QXDM-1854	Multiple GNSS views again not update	QCT Location Technology SCL	
QXDM-1698	Add Dynamic Item View to QXDM4	QCT Applications Engineering SH	
QXDM-1828	LTE Serving Cell display issue with SCC SNR	External	
QXDM-1815	QXDM display update request for new version 11 in log 0x147B	QCT Location Technology SCL	
PHONETOOLS-5831	Inconsistent arrow key behavior	Internal	
QXDM-1828	Radar 30516829 - QXDM4	QCT Applications Engineering - 01 SCL	
QXDM-1848	[Qxdm-4]Logging Bins seems to be missing on qxdm displays	QCT QST MST SD	
QXDM-1885	[case: 02828625]QXDM4->"LTE ML1 Serving cell Measurements Display" graphic not continuous	QCT Applications Engineering SH	
QXDM-1244	About Log Format	QCT Applications Engineering SH & TWN	
QXDM-1908	Item View - Cant Unhide hidden field	QCT Applications Engineering SH & TWN	
QXDM-1903	[VIVO] F11 hide payload, re-filter, payload unhide at re-filter windows	QCT Applications Engineering SH	

Latest QXDM Professional Software Version 04.00.00162 (2/23/2017).

•	New Features: 
•	Add version 34 of "LTE PDCCH-PHICH Indication Report" (0xB134) packet
•	Add version 7 of "LTE Random Access Request (MSG1) Report"
•	Add version 34 of "LTE ML1 QED Statistics" (0xB1D8) packet
•	Split the Debug messages in 3 columns
•	Added Online, FTM, EDL to Option Menu
•	Add version 33 of "LTE ML1 AdvRx IC Cell List" (0xB18F) packet
•	Add "LTE NB1 ML1 RLM Report" (0xB249) packet
•	Add 0x9400 (Pdsch_KPI_Report) with header_version v1/v2 & packet_version v1 under "UTRAN" -> "TBS" -> "RTF"
•	Bug Fixes: 
•	Fix for LTE NAS OTA parsing issue
•	Removed unneeded RequestNamedItem in Script helper.
•	Refresh graph immediately when scrolling using keyboard arrow keys.
•	Fix for repeated generation of ISF files due to invalid item count check even when not connected to device
•	Fixed automation logic for checking port connection state
•	Fix for GetItemWithClient Autonmation api call to return NULL object if invalid index.
•	Missing data in plots when selecting the cursor
•	Fixed for Default CFG read issue using CFG generator.
•	Resolved following JIRA tickets:
JIRA	Title	Raised by	
QXDM-1785	Updated: RE: Blocking: LTE Cat-NB IODT E/// UE issue 25: UE does not correctly advertise control plane CIoT EPS	NB1.MST	
QXDM-1724	remove RequestNamedItem & RequestNamedItemFile from Script helper.	CE	
QXDM-1244	About Log Format	QCT Applications	
QXDM-1681	LTE RRC State Plot Change functionality	QCT Applications	
QXDM-1852	QXDM Creating isf files infinitely on launch	QCT Applications	
QXDM-1847	QXDM : SendScript API issue	QCT Modem SW - I&T SD	
QXDM-1845	NV453 NV read issue with QXDM4.0.159 and 161	MST	
QXDM-1782	Commented: LTE plots are choppy	External	

Latest QXDM Professional Software Version 04.00.00160 (2/14/2017).

•	New Features: 
•	Add version 2 of "RF ASDIV" (0x1841) packet
•	Add following new versions in mac packets(0xB060 & 0xB061): Version 3 of SubPacket ID 2; Version 6 of SubPacket ID 3; Version 3 of SubPacket ID 4; Version 3 of SubPacket ID 5;
•	Added following messages:  GSM Immediate packet assignment; System information type 21; System information type 22; System information type 23
•	Add version 3 of Sub packet 25 into "Srch TNG Asdiv" (0x11A6) packet
•	Added following (internal) packets and versions: "LTE NB1 FW EFS" (0xB202); "LTE NB1 FW DRX" (0xB203); "LTE NB1 FW DL Measurement" (0xB215); Version 2 of "LTE NB1 FW Search PSS Auto Corr Result" (0xB208); Version 2 of "LTE NB1 FW Search PSS XCORR FFT Result" (0xB20B); Version 2 of "LTE NB1 FW DL Channel Estimation" (0xB211); Version 2 of "LTE NB1 FW DL TL" (0xB213); Version 2 of "LTE NB1 FW DBack NPDSCH Decode Result" (0xB228)
•	Add version 128 of "LTE LL1 Serving Cell RS" (0xB134) packet
•	Added Graph in TaskProfiling MPU view
•	Added Saving DIAG Task Profile Requests
•	Add version 26 of "LTE LL1 PDSCH Demapper Configuration" (0xB126) and version 24 of (Internal) "LTE LL1 MPDCCH Chest Demod" (0xB145) packets
•	Add version 122 of "TDSCDMA L1 DL FW DPCH PCCPCH SCCPCH Decode Result" (0xD01F) packet
•	Add many ONE-WEB packets
•	Added 9 new SSID messages
•	Depreciated Power SAR display
•	Added New Displays: Power SAR History, Power SAR Transmitter 0, Power SAR Transmitter 1, Power SAR Transmitter 2, Power SAR Transmitter 3
•	Added DPL view
•	Bug Fixes: 
•	Fixed "APN AMBR IE" in  Activate default EPS bearer context request messaage
•	Fixed ExportViewText to print summary text for events
•	Increased the default range of x-axes in LTE VIDE RTP Data Rate Packet Rate display
•	Fixed the 'length' of 'Header compression configuration' IE
•	Fixed 0x1476 field name issue
•	Fixed GNSS Position Display exceptions
•	Fixed stability issues related to MultiSIM functionality
•	Fixed error when sending SPC code
•	Resolved following JIRA tickets:
JIRA	Title	Raised by	
QXDM-1755	Message View Information when extracted to text file	QCA CNSS MCL BT/FM System Test SD	
QXDM-1778	QXDM 4 unable to restore saved configuration for LTE Video RTP Data Rate Packet Rate window.	QCT QST MST SD	
QXDM-1530	Add Graph in TaskProfiling MPU view	QCT SW CE EngOps TWN	
QXDM-1653	Add Saving DIAG Task Profile Requests	Unknown	
QXDM-1811	GNSS Position Report Display errors	QCT SW CE EngOps TWN	
QXDM-1786	QXDM4.0.157 keeps crashing with MultiSIM enabled - Blocking.	QCT WT Modem SW Applications Engineering SCL	
QXDM-1790	Enhancements to Power SAR display	QXDM Internal	
QXDM-1442	Add DPL view in QXDM4	QXDM Internal	
QXDM-1825	SPC 000000 not working on QXDM4	QCT QST MST SD	

Latest QXDM Professional Software Version 04.00.00158 (2/3/2017).

•	New Features: 
•	Added new automation API IsModemEFSReady() to check the modem NV/EFS ready states
•	Several updates to default DMC
•	Added new automation API SearchForEventOccurrences() to match all events matching a given Event ID
•	Bug Fixes: 
•	Fixed horizontal scrollbar step size in QXDM Window
•	Fixed parsing of "WCDMA Uplink and Downlink Power Control Edition 2" (0x4023) packet
•	Fixed a memory leak in HTML displays
•	Fixed "LTE ML1 Connected Mode Measurement Configuration" (0xB177) sub packet "Conn Meas Config Bitmasks" (id 37)
•	Fixed logging interruption after Alt+L
•	QXDM now saves the configured "Log File Path" in DMC, and loads the same from DMC
•	Add version 124 of "LTE LL1 Rx On Toggle Info" (0xB136) packet
•	Add version 2 of "IMS Video Encoder" (0x1752) and version 4 of "IMS Video Playout" (0x1753)
•	Fixed bug where NV Browser buttons would remain enabled after disconnecting DUT
•	Added auto scroll indicator to item views and filter views
•	Add version 2 of 0x1384
•	Improved robustness of HTML displays, so an exception in a single display will not block all displays
•	Prevented opening a second instance of the same HTML display
•	Add version 5 of "GSM LIF Metrics" (0x509F) packet
•	Fixed bug where QXDM would not exit properly when started via automation
•	Renamed "Quick Search" to "View Finder" and added more space between "Command" box and "View Finder" box 
•	Add "MCS CXM Metrics Info" (0x19C2) packet
•	Add 0x41AA (WCDMA DRX PICH Log Packet) v7
•	Updated Item View and Filtered View to save size of Items List window and Parsed o/p Window to dmc
•	Added enhancement of vocoder statistics view related with EVS, G711
•	Resolved following JIRA tickets:
JIRA	Title	Raised by	
QXDM-1720	Problem with parsing 0x4023	QCT WT Modem SW Applications Engineering SCL	
QXDM-1073	RE: QXDM memory problem as explained today	Nomad SW Eng	
QXDM-1729	QXDM Release x64 Needed	Nomad SW Eng	
QXDM-1731	QXDM4 (v153): F3s stop showing up in Log View Window after Logging Stop/Start (Alt+L)	QCT QST MST SD	
QXDM-1722	IsModemEFSReady()	QCT QST MST SD	
QXDM-1541	QXDM log location	QCT QST MST GRMNY	
QXDM-1639	QXDM4 "NV Browser" button still enabled when disconnect DUT	QCT Applications Engineering SH	
QXDM-1670	auto scroll indicator	QCT SW CE EngOps TWN	
QXDM-1423	QXDM4: Optimization for OTA log packets default parsing view	QCT QST MST HYD	
QXDM-1748	GNSS views not updated	QCT Location Technology SCL	
QXDM-998	RE: Perl scripts and QXDM4	QCT Location Technology SCL	
QXDM-1764	QXDM UI modification requests	Qualcomm Reference Design QRD	
QXDM-1711	RE: EVS, G711 vocoder packet statistics in Vocoder statistics view - QXDM 4	QCT APTech Audio SW HYD	
QXDM-1466	[LeTV] QXDM4 horizontal scroll bar's step too large	QCT Applications Engineering SH	

			

			

QXDM Professional Software Version 04.00.00157 (1/25/2017).
       - New Features:
Add version 2 of "RT-SAR Log Frame" (0x194E) packet
Add version 16 of "LTE RRC MIB Message Log Packet" (0xB0C1) packet
Add "LTE NB1FW DL Demod Summary" and "LTE NB1FW DL TTL Vs Time" analyzers

       -Resolved following JIRA tickets:
JIRA	Title	Raised by	
QXDM-1695	Fixed device connect issues with automation after device reset.	MST automation	
QXDM-1372	Added automation interface versioning. New automation APIs will only be added to AutomationWindow2 interfaces.	KPI 	
QXDM-1676	Added missing GetItemSpecificTimestamp2() for HTML view	MST Field testing 	
QXDM-998	Added SetQXDMInSingleInstance automation API	GPS	
QXDM-1657	Set the default font to be the same as QXDM3 for ItemView and Filtered View.	External	
QXDM-1252	Splitting date and timestamps into different columns	MST_TDSCDMA

QXDM-1541	Fixed issue about log location setting.
	MST GRMNY	

QXDM Professional Software Version 04.00.00155 (1/20/2017).

Fixed a crash issue related with certain display. QXDM-1620.

QXDM Professional Software Version 04.00.00152 (1/18/2017).

Bug fixes to relax validation on enum values in NV browser
Bug fixes to display javascript errors in HTML displays
Bug fixes to save 'user-defined html' views in DMC configuration
Fixed an issue to allow saving user html view in DMC and restore later
Moved column state settings from QSettings into DMC
Fixes for QXDM title bar
Enabled Javascript and HTML debugging
Added static EFS view
Added QXDM Tag Settings
Fixes to correctly save log mask in DMC file
Fixes for WaitEvent automation API
Made Status Bar on bottom of QXDM window configurable
Added highlight for search string in Match dialog
Added "No Connection" status display to NV Browser dialog
Changed default font to SegoeUI
Added functionality to disconnect from and reconnect to device after the target is refreshed
Fixed decoding of ASN.1 PDU

Latest QXDM Professional Software Version 04.00.00150 (1/9/2017).

Bug fixes for item list config dialog
Updates for APR parsing
Added GUID information in Device Information View
Added copy feature for NV browser
Bug fixes for LTE RRC parsing
Bug fixes for Export View Text
Added support to load "dmc", "hdf", "bin", "dlf", and "qmdl" in File->Open dialog
Bug fixes for GNSS Database display
Bug fixes for QXDM Status bar when loading ISF
Bug fixes for RecordBuilder
Bug fixes for creating NV buffer
Fixes to Load DMC file on a double click
Bug fixes for device connection issues

Latest QXDM Professional Software Version 04.00.00148 (12/15/2016).

Updates to Default.dmc
Added UIM State View
Fixes for Refiltered View Configuration
Fixes for displays: GNSS Position Report, GNSS Navigation Database, WCDMA Temporal Analyzer and Pilot Scanner, GSM 2G 3G Serving and Neighbor Cell Information
Added new Diag Subsystem command to retrieve and display model id
Fixes to display multi-sim 0xB0C0 packets
Moved "Close" and "CloseAll" later in the Window dropdown
Fixes to Automation interfaces NV read and NV write
Added Auto-Scroll All feature
Fixes for dynamic parser
Added support for GSM OTA parsing
Added Utilize Categories in Configuration View
Added automation APIs to convert back and forth from dmc to cfg files
Fixes for display update after saving
Fixes for saving ISF at the configured path
Fixes to make C++ automation consistent with other automation types
Added Load QDSS BIN file feature
Added generic open file dialog
Fixes for DPL protocol
Fixes for ADPL logging status timer on device reset
Added support for DIAGIN files
Fixes for Bookmark Up/Down in filtered view
Removed link to unexposed functionality for external release

Latest QXDM Professional Software Version 04.00.00146 (12/06/2016).

UI improvements for Highlight Dialog
Stability fixes
Fixes for NV command interface
Fixes for ISF setting page layout
Added Highlight persistent mode
Fixes for QCAT Format parsing option
Fixes for SD Logging save a load cfg
Fixes for NV automation
Fixes for filtering items in automation
Fixes for APR parsing

Latest QXDM Professional Software Version 04.00.00144 (11/21/2016).

Bug fixes for NV Browser
Bug fixes for Tile Horizontal feature
Stability Fixes
Fixes for parsing of LTE OTA packets
Fixes for log size after port disconnect
Fixes for C++ automation
Added app signing for the QXDM installer
Fixes for Item View
Fixes for Find Next/Previous functionality
Fixes for C# automation
Fixed displays: LTE ML1 SCell State Change display, CDMA Temporal Analyzer, LTE Carrier Agg Summary
Fixes for Clear All functionality
Fixes for Logkit Conversion
Fixes for running on XP machine
Added Highlight feature

Latest QXDM Professional Software Version 04.00.00142 (11/07/2016).

Bug fixes for NV Backup and Restore
Bug fixes for OTA log direction prints
Bug fixes for Item View
Added display: MLOG Memory Profiling
Added "Clear" option to the context menu for plots
Bug fixes for "Show Legend" function
Added menu items to launch PPP extractor and Diag DB editor
Added function to convert QSH trace messages into standard debug messages
Added "Compact Layout" function to Replay dialog
Stability Fixes
Added automation APIs for GPS Info
Added Multi-SIM support for Filtered Views
Bug fixes for "Find Next" and "Find Previous" functionality
Bug fixes for Bookmark sync to item
Added functionality to associate QXDM4 with .dmc and .isf files
Bug fixes related to third party DLLs
Fixed displays: GNSS Position Report, GNSS Clock Report, GNSS GAL Measurements, LTE ML1 DL Throughput and Bler
Added feature to automatically populate several fields in QLMS activations 

Latest QXDM Professional Software Version 04.00.00140 (10/25/2016).

Bug fixes for filter view
Stability fixes
Added support for delayed response in automation api
Bug fixes for bookmark up and down functions
Bug fixes for Status (Dynamic) window
Bug fixes for call manager

Latest QXDM Professional Software Version 04.00.00138 (10/23/2016).

Fixed displays: LTE Video DL RTP Jitter, LTE Video RTP Data Rate Packet Rate, LTE Video RTP Payload Size Error Rate, LTE RLC Throughput graph, LTE ML1 DL Throughput & BLER, LTE ML1 UL Throughput & BLER, WCDMA Pilot Scanner, LTE ML1 Serving Cell Measurements
Added LteRrcVD21 for B0C0 parsing support for version 15
Chart background color changed to black
Bug fixes for NV Browser
Bug fixes for command output
Bug fix for lost logging on device reboot
Performance improvements
Added "Find Previous" function to Item View
Added displays: Task Profiling MPU and Temperature Monitor
Fix for memory leak in automation

Latest QXDM Professional Software Version 04.00.00135 (10/11/2016).

Fixed display: LTE ML1 SCell State Change
Added Copy to Clipboard feature
Added Export Item View Contents feature
Added Bookmark feature
Added LteRrcVD21 for B0C0 parsing support for version 15

Latest QXDM Professional Software Version 04.00.00133 (09/23/2016).

Added display: HDR Pilot Sets
Added Subsystem V2 diag request/response support
Add support for user parser dlls
Added support for GetAPSWindow
Added feature to copy NV field values row in NV Browser
Added Export text to file feature
Fixed QXDM title issue
Fixed displays: Device Information, LTE PDCP DL Throughput, LTE RRC State Change Plot, LTE RRC NAS Status Screen
Fixed WaitForItem command interface method
Fixed Quick Search scrolling
Fixed Manage Config's Save As Dmc & Save As Txt options
Support in QXMD4 to enable Modem and stm data
Fixed updating the programName for the Logkit Converted file
Fixed sync between Item View and Command Output
Fixed ClientRequestNVRead/Write multi-sim context_xx
Updated IDL for automation

QXDM Professional Software Version 04.00.00131 (09/23/2016).

Fixed display: LTE ML1 DL Throughput and BLER
Add "Config with Registrations" option in Filtered View context menu

QXDM Professional Software Version 04.00.00127 (09/16/2016).

Fixed display:  GSM 2G/3G Serving And Neighbor Cell Information, LTE IMS VoLTE Status, CGPS Control, GNSS Fix Collection
Fixed Command Output
Fixed NV Write
Fixed QXGPS registration
Fixed tlb COM issues 
Fixed Sahara device crash

QXDM Professional Software Version 04.00.00125 (09/09/2016).

Added support for RRCVAB1, RRCVC80, RRCVD20
Fixed display:  LTE CER RX Tx Pair, Status (Dynamic)
Fixed search/match options in item/filtered views

QXDM Professional Software Version 04.00.00123 (09/01/2016).

Fixed database

QXDM Professional Software Version 04.00.00121 (08/25/2016).

Added display: MSIM Mode Of Operation Real Time
Added loadSettings and saveSettings for ULog Viewer
Added separate column settings for Filtered View, Log View and Message View
Added Diag Req/Rsp based ULog support
Remember table settings in graph displays
Sync master hash file of QShrink
Fixed display: Call Manager, LTE ML1 DL Throughput and BLER
Fixed malformed QDSS
Fixed Command Output
Fixed issue that one ULog item has multiple parsing processes
Fixed tile horizontal option
Fixed log 0xB193 handling issue
Fixed filtered view position persistence
Fixed QXDM-QTF server crash
Cleaned up displayed GPS devices
Cleaned up unused menus

QXDM Professional Software Version 04.00.00119 (08/10/2016).

Added display: Qurt Performance Monitor
Added "Dip Switches" option
Added "Reset Application Settings" option
Added zipping ISF feature
Enhanced meta data info of device build
Enhanced command output performance
Fixed display: GSM Power Scan Results, WCDMA Pilot Scanner
Fixed TCP device crash
Fixed QDSS support
Fixed ULog behavior
Fixed saving .cfg file
Fixed subsystem command configuration
Fixed APR parsers
Fixed 0x412F parsing
Fixed GetItemSummary for debug messages
Fixed windows dropdown
Fixed minimum window size

QXDM Professional Software Version 04.00.00117 (07/26/2016).

Added display: GSM GPRS Information, GNSS QZSS SBAS Measurements
Fixed display: LTE ML1 Uplink Tx Display
Fixed filtered view configuration issue
Fixed windows dropdown
Fixed minimum window size

QXDM Professional Software Version 04.00.00115 (07/26/2016).

Added new High Data Rate (HDR) file format in QXDM
Added displays:  QuRT ADSP Performance Monitor, QDSP6 QuRT Thread Profilor - ADSP, QDSP6 QuRT Thread Profilor - MPSS
Added item list font settings
Added meta data info of device build
Improve SendScript and implement SendCommand automation methods
Updated Default DMC to Version 3
Added Secondary DMCs: DPLFull.dmc, CnEMessageAll.dmc, DPMMessageAll.dmc
Added Default.cfg
LinuxDataMessageAll.dmc
Fixed displays:  LTE ML1 Real Time RSRP, LTE ML1 PMCH Throughput and BLER, NV Browser,  WCDMA State Transition Power, L3 Signalling Messages, E-FACH Feature, several HTML-based displays
Fixed Match on Log View
Fixed log packet selection when using ALT+L
Fixed qshrink4 downloading
Fixed Item/Filtered View UI
Fixed Computer ID issue
Optimize Logkit conversion

QXDM Professional Software Version 04.00.00113 (07/11/2016).

Added displays:  WCDMA+ TTI State, WCDMA L3 Signaling Messages, WCDMA E-FACH Feature, WCDMA State Transition and Power
Added Diag DB Editor
Added annotations in command output
Added automation method: GetFieldType
Added automation samples
Added Generic Menu option to use External DLL for parsing
Sync master hash file of QShrink 
Fixed displays: LTE LL1 CER Rx-Tx Pair, LTE LL1 CQI RI MCS, LTE ML1 DL Throughput BLER, LTE ML1 Serving Cell Display, LTE ML1 Serving Cell RSSI SINR, LTE ML1 Serving Cell NVDVGA, NV Browser, Status (Dynamic)
Fixed Find and Match progress dialog
Enhanced performance for saving log view

QXDM Professional Software Version 04.00.00111 (06/27/2016).

Added displays: CGPS NMEA Control, GSM EGPRS Uplink/Downlink Quality, WCDMA+ Configuration, WCDMA+ Mode Information
Added GPS support in automation interface
Added support for 0x1386 and 0x1387 LSM Report Service
Added persistence to replay dialog
Added F5 shortcut key for Log View config dialog
Enhanced Find/Match support
Improved options for QShrink4 warnings
Fixed displays: GNSS Position Report, GSM 3G Neighboring Cell Info, NV Browser
Fixed timestamp issue that it was always showing item-specific timestamp for Log/Event/Messages
Fixed GSM OTA items arriving
Fixed DMC and CFG load issue
Fixed "Alt+S" not working in ItemView/filtered View
Fixed RequestNVItemWrite and RequestNVItemRead support in command bar
Fixed printing Diag RX items in Command Output Window
Other performance and UI improvements

QXDM Professional Software Version 04.00.00109 (06/13/2016).

Added display: LTE LTED Scheduling Pattern
Added QDSS automation support
Improve UI spacing
Fixed displays: GNSS Measurements, GNSS TDP Measurement, LTE Direct Configuration, NV Browser, WCDMA Temporal Analyzer
Fixed OTA color in ItemView
Other performance and UI improvements

QXDM Professional Software Version 04.00.00107 (06/06/2016).

Add displays: GSM GPRS TX Timing, CRAT displays, LTE Direct Configuration,  GPS NMEA Control
Update automation samples
Fixed displays: Active Set Information, CDMA Pilot Information, CDMA Power, GNSS Measurements, GPRS Serving Cell Parameters, LTE ML1 TuneAway Graph, NV Browser, WCDMA Power Control, WCDMA EUL Link Measurements, WCDMA HSDPA Link Statistics,  WCDMA Temporal Analyzer
Fixed connection dialog
Fixed close device issue
Fixed ClearViewItems automation method
Fixed Export Item View, Message View 
Fixed DPL crash issue
Fixed window scrolling issue
Fixed crash caused by automation QuitApplication 
Fixed automatic ISF naming entry
Fixed duplicate windows when loading dmc

QXDM Professional Software Version 04.00.00105 (05/23/2016).

Add new displays: WCDMA BLER, WCDMA BLER Total
Enhanced connection dialog to support independent GPS connections
Updated new timeline feature
Updated automation demo
Fixed displays: GSM 2G 3G Serving And Neighbor Cell Information, GSM 3G Neighboring Cell Information, LTE ML1 Acquisition PBCH Serving Measurement, LTE PDCP Config, LTE RLC Config, LTE RLC Statistcs Screen, LTE RRC NAS Status Screen, NV Browser, TDSCDMA MAC Parameters
Fixes NV write 71527 where uint16 is not converted correctly causing wrong value being written to EFS
Fixed device reset and auto reconnect issue
Fixed TRM parser
Fixed GetSummary automation method
Fixed automation issues with Perl
Fixed graph control
Fixed window visibility
Fixed QDSS support

QXDM Professional Software Version 04.00.00105 (05/16/2016).

Added C# automation sample
Update TRM parser
Fixed displays: LTE ML1 DL Throughput And BLER, LTE ML1 UL Throughput And BLERLTE ML1 Serving Cell Measurements Display, LTE ML1 Serving Cell LNA VGA, LTE ML1 Serving Cell RSSI SINR, NV Browser, WCDMA Power Contro
Fixed automation interface
Fixed NV read/write
Fixed plot update issue
Fixed browse to ISF directory in Item store settings 
Fixed issue connecting to device with Dynamic Status display opened
Fixed load/save DMC files
Fixed Clear All issue
Fixed CFG File Generator
Fixed QDSS QTF feature

QXDM Professional Software Version 04.00.00101 (05/09/2016).

Added option for QCAT parsing format
Fixed displays: GSM 2G/3G Serving And Cell Information, GSM Surrounding Cells,  LTE ML1 Real Time RSRP, LTE ML1 Serving Cell Measurements Display, LTE ML1 Serving Cell LNA VGA, LTE ML1 Serving Cell RSSI SINR, WCDMA Pilot Scanner
Fixed graph cursor issue
Fixed graph frozen issue
Fixed command output view appearing
Fixed event summary parsing
Fixed the memory issue related with Events buffer in Automation

QXDM Professional Software Version 04.00.00099 (05/02/2016).

Added cursor to all graphs
Fixed displays: GSM Power Scan Results, NV Browser, LTE ML1 DL Throughput and BLER, LTE ML1 Serving Cell Measurements, LTE ML1 Real Time RSRP Neighboring Cell,  LTE VoLTE IMS Status,WCDMA NAS Mobility Management, WCDMA Power
Fixed send command crash
Fixed NV write issue
Fixed selection of OTA log ids in Fitered View
Fixed graph timeline
Fixed QTF server support

QXDM Professional Software Version 04.00.00097 (04/22/2016).

Added support for DMC Display Positions
Added support for Filter-On-String
Added standard windows menu keyboard navigation with Alt key
Added Sub ID column to item views
Added TRM Service
Updated LTE RRC parser version to use Vc7 dll.
Added displays
GSM EGRPS Uplink BSN Arrival
GSM EGRPS Downlink BSN Arrival
GSM Random Access Attempts
Fixed displays: LTE ML1 Serving Cell Measurements, LTE ML1 Serving Cell RSSI SINR, LNA, DVGA, LTE ML1 Real Time RSRP, LTE ML1 UL Throughput and BLER, LTE DL Throughput Estimation
Fixed GPS error handling
Fixed DPL issues
Fixed command output window
Fixed graph charts overlapping
Other performance and UI improvements

QXDM Professional Software Version 04.00.00095 (04/18/2016).

Split "GSM GERAN Burst Metrics Display" to two displays: "GSM GERAN Burst Metrics Display" and "GSM GERAN Burst Metrics CRC Display"
Fixed displays:
GSM GPRS Air Interface Summary
GSM Power Scan Results
LTE ML1 DL Throughput and BLER
LTE ML1 Uplink Tx Display
LTE LL1 SNR CQI RI MCS Display
LTE Video RTP Data Rate Packet Rate
Fixed automation methods: ClientRemoveRequest, RemoveRequest and RequestItem
Fixed malformed items
Fixed nv values being reverted upon device reset
Other performance and UI improvements

QXDM Professional Software Version 04.00.00093 (04/11/2016).

Added Log View and Message View. They can be configured using context menu option. The Log View save path can be specified in the ItemStoreSettings.
Added "Discovered Items" feature
Added hardware dongle support (Windows only)
Enable Log 0x1951 whenever Log 0x11EB is set
Fixed displays:  
GSM 2G 3G Serving And Neighbor Cell Information
GSM 3G Neighboring Cell Information
GSM Dedicated Mode WCDMA Cell List
LTE ML1 Serving Cell Measurements
LTE ML1 Serving Cell RSSI SINR
LTE ML1 Serving Cell LNA DVGA
LTE LL1 CQI RI MCS Display
NV Browser
Fixed copy items to ISF option
Fixed graphing component
Fixed automation API issues
Fixed DMC loading
Fixed QShrink4 issues
Other performance and UI improvements

QXDM Professional Software Version 04.00.00091 (03/30/2016).

Updated settings dialog
Updated DPL support
Updated WCDMA/TDSCDMA RRC Accumulator
Updated QShrink hash file
Fixed hexadecimal entry support in NV Browser
Fixed memory issue when opening multiple filtered views
Fixed calculations for LTE ML1 Real Time RSRP display
Fixed issue for independent ISF configurations
Fixed save item store on exit
Fixed WCDMA 0x421F parsing issue
Fixed displays: Call Manager, GSM AMR Information, GSM Channel Parameters, LTE LL1 eMBMS, 
Fixed m-sim EFS NV access
Optimized GetName and SendDmIcdPacketEx automation methods
Other performance and UI improvements

QXDM Professional Software Version 04.00.00089 (03/22/2016).

Added Appearance Dialog
Added Annotate Menu
Added string item to end of ISF when saving
Added ability to create a timeline from a filter view
Added support for regex into user defined views
Added displays:  IPA Throughput And Drop Rate Mbps, IPA Throughput And Drop Rate Pps, LTE LL1 eMBMS SNR, LTE VoLTE Handover Delay/Interruption, TDSCDMA TTL Results
Added back missing WCDMA and GPS HTML displays
Fixed printing of complete file names for message packets 
Fixed text in summary column for Events
Fixed hide coulmns option in ItemView
Fixed multi-SIM support in NV Browser
Fixed Call Manager display
Fixed SaveConfig and LoadConfig automation APIs
Fixed cursor for QPlot graphs
Fixed QShrink4 exception handling and optimized loading process
Other performance and UI improvements

QXDM Professional Software Version 04.00.00087 (03/10/2016).

Add support to QLMS for proxy server

QXDM Professional Software Version 04.00.00085 (03/04/2016).

Added Command Bar methods and refined Command Output
Added "Refresh Target" and "Set Target Offline" functions under Options menu
Added Restore All windows menu feature
Added Cursor to some graph displays
Updated Power SAR display for log packet change
Fixed QSHRequest command bar method
Fixed QShrink4 database loading, status, and multi-session issues
Fixed a memory leak for DPL
Other performance and UI improvements

QXDM Professional Software Version 04.00.00083 (02/19/2016).

Added option in Communications dialog to turn on QPST's port trace
Added "Copy Headline To Clipboard" context menu option to Item View
Enhanced LTE Sleep State view UI
Added automation methods: IsQShrink3DBReady, IsDatabaseReady, IsQXDMSeeingThePortInQPST, IsQXDMAlreadyUsingThisPortInAnotherQXDMWindow
Increased y-axis range for UL Throughput display
Fixed NV read failures
Fixed ExportViewText and ClearViewItems automation methods
Fixed WCDMA HSDPA Link Statistics and  WCDMA HSDPA Decoding Staticistics view for newer log versions
Fixed a failure to reconnect to device via automation
Fixed an issue when loading a DMC
Other performance and UI improvements

QXDM Professional Software Version 04.00.00081 (02/11/2016).

Enhanced Item View column selections
Fixed LTE RRC parsing (OTA 0xB0C0) error by adding support for version 0xB0704
Fixed an auto-save issue
Other performance and UI improvements

QXDM Professional Software Version 04.00.00079 (02/09/2016).

Added GPS port selection
Added list of open windows in Window menu option
Added LTE ML1 Sleep State display 
Added LTE NAS support for B0E2, B0E3, B0EC, B0ED
Enhanced window visibility
Enhanced Call Manager display 
Fixed event format string in item view summary column
Other performance and UI improvements

QXDM Professional Software Version 04.00.00077 (01/27/2016).

Added PMIC Dashboard display
Added Command Bar methods: RequestItem, RequestNamedItem, QSHRequest
Enhance TDSCDMA Power 2
Enhance UMTS Cell Selection
Enhance device connection within automation
Added LTE RRC 0xB0C0 support for versions 11-13
Fixed Item View problem stalling with status commands
Fixed a crash issue when closing the WlanSignalStrength display
Other performance and UI improvements

QXDM Professional Software Version 04.00.00075 (01/20/2016).

Added Command Output Window
Added LTE OTA Parsing libraries VC74, VB74, VB73
Added Show All X Axis option to graph context menu
Added Reset Target menu function under "Options"
Added NV browser pull down menu support for enum fields
Enhanced clear item functionality in Item View and Filtered View
Fixed and enhanced several displays
Fixed Subsystem Diag command mapping
Other performance and UI improvements

QXDM Professional Software Version 04.00.00073 (01/15/2016).

Enhanced Call Manager with no UI updates until call originated. 
Enhanced NV Browser search functionality.
Enhanced Power SAR display.
Added the current COM Port to the title bar.
Fixed SendRawRequest command bar option.
Fixed key up/down and page up/down in Item View.
Fixed graph crash issue due to empty tables after reset.
Fixed crash issue opening some graph displays.
Fixed crash for TDS Power and Power 2.
Fixed Item View crash issue.
Fixed crash when connected devices were switched.
Other performance and debugging info improvement.

QXDM Professional Software Version 04.00.00071 (01/08/2016).

Added the “Vocoder Statistics” HTML display.
Added “Clear All” menu function.
Fixed issue that in Configuration View, “Task manager Services” not existed, SNS/LK has wrong items.
Enhanced Graphic display “LTE ML1 TuneAway” with new design.
Usability optimization and improvement in graphic displays. Allowed user to hide table, or certain charts. Reduced the minimal size of graphic display so user can have more displays to view at the same time.
Fixed issue related with QDSS+MSIM.
Enabled the Read/Write button when open NV browser with device connection.
Fixed issues related with F3 message processing with QSR3.
Fixed issues related refiltering items in ItemView and FilteredView.
Fixed issues that “clear items” didn’t work after replaying.
Fixed issues with “clear item”.
Fixed an issue that after open isf multiple times, too many QXDM windows opened.
Added several more graphic displays including CDMA Pilot Information.
Fixed issue on the LTE LL1 CER RX TX Pair display.
Added version 6/7 support for GNSS Search Strategy Task Allocation display. 
Fixed issue with GetFieldValueText in HTML displays.
Fixed issues with multi-x axis displays
Fixed an issue that after open isf multiple times, too many QXDM windows opened.
Other performance and debugging info improvement.

QXDM Professional Software Version 04.00.00067 (12/18/2015).

Added multi cells support for the LTE ML1 Serving Cell Measurement display.
Added “Vocoder Statistics” for log 1804 and 1805. 
Added more graphic displays, like LTE Estimation, HDR Air Link Summary, WCDMA Power Control and many others.
Performance improvement on HTML displays.
Fixed a UI hang issue when have both NV browser and filtered view open with F3 message.
Fixed OTA parsing
Fixed automation API issue related with NV read/write.
Fixed several graphic displays issues in step charts.
Added new version support for LTE ML1 DL Throughput BLER display.
Other performance and UI improvements

QXDM Professional Software Version 04.00.00060 (12/1/2015). internal build.

Added timeline tool
Added and enhanced several graphic displays
Enhanced splash screen
Fixed auto scrolling across multiple plots
Fixed Replay Dialog
Fixed OTA parsing
Fixed an issue when opening a second isf
Fixed device crash on device plug-out during connection
Fixes LTE ML1 Seving Cell Measurements display
Fixed VoLTE RTP Payload Size and Error Rate display
Other performance and UI improvements

QXDM Professional Software Version 04.00.00060 (11/20/2015). external build.

•	Same build as internal 59.

QXDM Professional Software Version 04.00.00059 (11/20/2015). internal build.

•	Added version 21 support for packet B193 in LTE ML1 Serving cell management display.
•	Added version 26 for LTE ML1 Uplink Tx display.
•	Fixed an issue when loading a DMC from QXDM3 to automatically generate Filtered View for “Log View” and “Message View”.
•	Fixed a UI hangs issue caused by javascript error in the WCDMA EUL E-TFI Usage display.
•	Fixed an issue that certain displays’s X_Axis was not scrolling.
•	Added “DEMO_MODE” in graphic displays XML definition to allow user quickly change fonts for demo purpose.
•	Added several graphic displays.
•	Other performance and UI improvements.

QXDM Professional Software Version 04.00.00055 (11/06/2015). external build.

•	Fixed issue for LTE ML1 UL Throughput Bler display.

QXDM Professional Software Version 04.00.00055 (11/02/2015). Internal build.

•	Added UI progress bar during QShrink4 F3 message conversion when open ISF collected from LogKit.
•	Added Secondary DMC and DMC library.

QXDM Professional Software Version 04.00.00054 (10/30/2015). Internal build.

•	Fixed stability issues related with graphic displays.
•	Added LogKit QShrink4 support.
•	Added several graphic displays.
•	Improved the performance of graphic displays with packet new parsing solution.
•	Added new packet version support for graphic displays.
•	Fixed issues with HTML displays.

QXDM Professional Software Version 04.00.00051 (10/16/2015). External build.

•	Fixed a crash issue related with device reset/disconnect/reconnection.
•	Added PDCP graphic display.
•	Added UDC graphic display.

QXDM Professional Software Version 04.00.00049 (10/02/2015). Internal build.

•	Fixed a crash issue related with a display LTE ML1 UL Throughput & Bler.
•	Fixed issue with automation API for Item Store Settings.
•	Improved the performance of graphic displays.
QXDM Professional Software Version 04.00.00048 (09/30/2015). Internal build.

•	Added more than 30 displays (LTE, TDSCDMA and WCDMA).
•	Added support for DMC conversion. When loading legacy DMC with LogView or MessageView Configuration, it will give option to create FilteredView with the same configuration.
•	Fixed issues related with automation APIs, and NV operations.
•	Fixed a crash issue when loading ISF with customers hash table.
•	Fixed an issue when doing “Match Items” on Filtered View.
•	Fixed a crash issue when receiving invalid packet in dynamic status display.
•	Improved the performance of graphic displays.
•	Added multi-SIM support for displays.
•	Added automation API for loading QShrink4 hash file.
•	Added automation API to set QShrink4 server path.

QXDM Professional Software Version 04.00.00046 (09/11/2015). Internal build.

•	Fixed the issue that when connected to second UE, no QXDM window was opened.
•	Fixed the Window title issue after connected/disconnected device.
•	Added graphic displays.

QXDM Professional Software Version 04.00.00045 (09/04/2015). Internal build.

•	Memory optimization and other performance improvement. 
•	Added NV R/W Automation APIs. Added Automation APIs for NV reading and Writing. Also includes various automation bug fixes.
•	Added several Automation APIs requested by APS team. 
?	Added get event summary API.
?	Added get event name API.
?	Added the get and set the ISF File size API. 
?	Added the DisconnectfromComport() API
•	Fixed an issue that after a device was connected, still be able to connect to it and create a new QXDM session.
•	Fixed a crash issue when running match items.
•	Fixed several Automation API issues.
?	PHONETOOLS-4672, GetFieldCount()
?	PHONETOOLS-4671, GetFieldIndexByID()
?	PHONETOOLS-4673,GetFieldIndex()
?	PHONETOOLS-4594 QXDM fails to connect
?	PHONETOOLS-4565,QXDM4 shows Incorrect COMPort Status.
?	PHONETOOLS-4670,&nbsp;GetConfiguredItemFields()()
?	PHONETOOLS-4669,&nbsp;ConfigureClient()()
?	PHONETOOLS-4625,CreateView()
?	PHONETOOLS-4619,Not able to reconnect the Device once we call Disconnect().
QXDM Professional Software Version 04.00.00041 (07/31/2015). External build.

•	Added QShrink4 support.
•	Added DPL support.
•	Added “Refilter Items” context menu function.
•	Added “REGEX” expression support for Find and Match.
•	Added “Heap Analyzer” display.
•	Added the function to gracefully disconnect from device.
•	Added the function to gracefully exit QXDM. Temporary ISF will be deleted when QXDM quits.

QXDM Professional Software Version 04.00.00040 (06/30/2015). External build.

•	Same as 00039, make it available for external customers.

QXDM Professional Software Version 04.00.00039 (06/30/2015). Internal build.

•	Fixed a crash issue when open NV browser for certain device.

QXDM Professional Software Version 01.00.00038 (06/29/2015). Internal build.

•	Improved performance, fixed memory leaks and fixed several issues in F3 message parsing, OTA message parsing.
•	Added Automation API support for Windows QXDM4.
•	Added QTF/QDSS integration to QXDM on Windows.
•	Added QLMS to QXDM. Users will need to activate their account before using QXDM.
•	Added VS2013 distribution package as part of the QXDM installation process on Windows.
•	Added primary (default) DMC, user can turn it on by click it on toolbar.

QXDM Professional Software Version 01.00.00036 (06/01/2015)

•	Added Context menu function “Bookmark”.
•	Added footer to show statistics data when collecting data from device.
•	Improved performance on Replay with “No Wait” configuration.
•	Fixed an UI hang issue during NV writing.
•	Fixed a crash issue during ISF saving.
•	Fixed memory leak when collecting data from device, optimized memory usage with QShrink3 hash table.
•	Fixed a UI issue in Item View when there are multiple windows opened.
•	Added index to filtered views to identify them.
•	Added user database path setting under “Parsing and DBs”.
•	Added user QShrink3 hash file location under “Parsing and DBs”. 

QXDM Professional Software Version 01.00.00035 (05/01/2015)

•	Added Context menu function “Match items”
•	Added Context menu function “Clear items”
•	Added Context menu function “Sync to item” and “Sync Near Item”
•	Added Context menu function “Time difference”
•	Improved performance on Context menu function  “Find” and “Find Next”.
•	Fixed an issue loading DMC file generated with old QXDM version.
•	Added user setting for “Item Store”
•	Added function to load user defined HTML displays. 
QXDM Professional Software Version 01.00.00034 (04/01/2015)

•	Same build as 00033 for internal customers.

QXDM Professional Software Version 01.00.00033 (04/01/2015)

•	Fixed a crash issue when there was a massive amount of traffic from the device.

QXDM Professional Software Version 01.00.00032 (03/31/2015)

•	Changed QXDM installer to support install overwrite at previous installed location.  
•	Added error handling in installer, show error messages and instructions whenever components failed to install.
•	Added Save ISF, New Items toolbar buttons for easy access to the functions.
•	Fixed bugs and improve performance.
QXDM Professional Software Version 01.00.00031 (02/27/2015)

•	Added function to load/save user configuration file (DMC).  
•	Added OTA Log Packets in Configuration View.
•	Added ISF file association with QXDM on Mac. ISF file will show the QXDM icon, and will be loaded when double click on the file. 
•	Added version info to the file name of QXDM installer. 
•	Fixed a UI stalled issue when collecting large set of data from high-speed device.
•	Added automation interfaces for Mac QXDM.
•	Added OTA messages parsing using RRC libraries.
•	Added OTA parsing using SILK on Mac platform.
•	Fixed several UI issues, updated replay toolbar icon.
•	Added latest GPS parsing support.
•	Changed location of application support folder to ~/Library/Application Support/QXDM for Mac.  ~/.config for Linux.
•	Changed database path to /etc/QUALCOMM/QXDM for both Linux and Mac.
•	Added NV backup/restore feature, with automation APIs supported as well. See sample script in NVBackup.pl and NVRestore.pl.
•	Changed the Hex view (bottom left) of Item view to separate the payload and binary data.
•	Fixed NV restore hangs issue for certain devices.

QXDM Professional Software Version 01.00.00030 (02/06/2015 Internal)

•	Added OTA Parsing using RRC libraries for both Linux and Mac.  
•	Added OTA parsing using SILK on Mac platform.
•	Added all HTML Display (125 displays) support for Linux and Mac. 
•	Fixed an issue that displays sometimes not showing result from replay. 
•	Fixed several UI issues, updated replay toolbar icon.
•	Added latest GPS parsing support.
•	Changed location of application support folder to ~/Library/Application Support/QXDM for Mac.  ~/.config for Linux.
•	Changed database path to /etc/QUALCOMM/QXDM for both Linux and Mac.

QXDM Professional Software Version 01.00.00029 (12/05/2014 Internal)

•	Addressed installer issue for Mac QXDM 00028 build.
•	Fixed an issue that temporary ISF was not generated properly during live data collection. 

QXDM Professional Software Version 01.00.00028 (11/29/2014 Internal)

•	Added NV backup/restore feature, with automation APIs supported as well. See sample script in NVBackup.pl and NVRestore.pl.
•	Added automation APIs support for Mac QXDM. Same script can work botn on Mac and Linux.
•	Fixed issue in Command box. Verified that commands like “mode offline-d”, “mode lpm” and “mode reset” work. 
•	Fixed an issue that “New Items” menu didn’t work.
•	Fixed an issue when save items to existing ISF files.

QXDM Professional Software Version 01.00.00027 (10/27/2014 Mac)

•	Fixed an issue that libusb was not installed properly for external customers.
QXDM Professional Software Version 01.00.00026 (10/24/2014 Mac)

•	Fixed an issue that NV browser didn’t work for devices without EFS turned on.
•	Fixed a crash issue when try to re-connect and device that already connected.

QXDM Professional Software Version 01.00.00025 (10/17/2014 Internal)

•	Fixed device name listed as “Android” issue.
•	Added version info to the Mac QXDM plist.
•	Added UI in Preferences=>USB to allow users adding new devices. If you have a device not supported by default, you can use this UI to add it so QXDM can communicate with the new device.
•	Fixed several Sahara crash dump issues.
•	Fixed devices detection issue on Mac.
•	Added NV backup/restore for internal users build. In testing status.
•	Added EFS Explorer for internal users build. In early development status. Can allow user to view the EFS in read-only mode in this build. More function is coming.
QXDM Professional Software Version 01.00.00024 (10/17/2014)

•	Fixed device name listed as “Android” issue.
•	Added version info to the Mac QXDM plist.

QXDM Professional Software Version 01.00.00023 (10/13/2014)

•	Added UI in Preferences=>USB to allow users adding new devices. If you have a device not supported by default, you can use this UI to add it so QXDM can communicate with the new device.
•	Fixed Mac installer issue that sometimes the libusb library was not downloaded.
•	Fixed several Sahara crash dump issues.
•	Fixed devices detection issue on Mac.

QXDM Professional Software Version 01.00.00021 (09/02/2014)

•	Fixed a crash issue when quit QXDM with device connected.
•	Updated QXDM application icon for Mac QXDM.
•	Fixed issues with NV browsers.

QXDM Professional Software Version 01.00.00020 (08/25/2014)

•	Externalized version of Release 01.00.00019, with proprietary functionalities disabled.

QXDM Professional Software Version 01.00.00019 (08/19/2014)

•	Added support for multiple devices with same Vendor Id, Product Id but different diag interfaces.
•	Fixed issues with NV browser related with reading/writing.
•	Added support for BroadMobi devices.
•	Added icons in user settings and application icons.

QXDM Professional Software Version 01.00.00017 (08/07/2014)

•	Added user space USB driver for Mac QXDM.
•	Added HTML displays for Mac QXDM.
•	Added icons in user settings and application icons for Mac QXDM.

QXDM Professional Software Version 01.00.00016 (07/17/2014)

•	Added support for selected Telit wireless devices.
•	Fixed several issues in NV browser.

QXDM Professional Software Version 01.00.00015 (07/07/2014)

•	Added support for selected LGE devices.
•	Added Call Manager display under Common menu. Currently, it works only with single call manager dialog opened. Multiple call manager dialog support will be in the future release.
•	Fixed several issues in Item View.
•	Fixed DMC related issue to save other displays info (like dynamic status display) info in DMC file and restore it later.
•	Fixed a crash issue when the application quit.

QXDM Professional Software Version 01.00.00014 (06/06/2014)

•	Added support for selected LGE devices.
•	Added Sahara software upload for flashless device.
•	Added more Automation Script interfaces with sample scripts. We now have 66 Automation APIs supported. For examples and details, please refer to /usr/QXDM/AutomationSamples.
•	Added more LTE/TDSCDMA HTML displays. 
•	Added more Context Menu functions in Item/Filtered Views.

QXDM Professional Software Version 01.00.00013 (05/02/2014)

•	Added support for selected Samsung and Google devices.
•	Added Context Menu in Item/Filtered Views.
•	Added more Automation Script interfaces with sample scripts. We now have 40 Automation APIs supported. For examples and details, please refer to /usr/QXDM/AutomationSamples.

QXDM Professional Software Version 01.00.00011 (04/18/2014)

•	Added support of DIAG over TCP/IP. Devices now can communicate with QXDM via TCP/IP connection. The default port is 2500. In the future, we will make the port configurable.
•	Sahara + USB improvements, Sahara crash dump download speed has been improved from hours to few minutes.
•	Added Compressed DIAG Interface. (Command code 0x9B)
•	Added EFS NV Files Probe and Alt File System support.
•	Added more graphic displays; we now have 20 graphic displays.
•	Added more Automation Script interfaces with sample scripts. We now have 30 Automation APIs supported. For examples and details, please refer to /usr/QXDM/AutomationSamples.

QXDM Professional Software Version 01.00.00010 (02/28/2014)

•	Sahara + USB improvements: added hot plug support
•	Initial EFS NV items support
•	Static Status screen 
•	Added Automation Script interfaces with sample scripts; more are coming.

QXDM Professional Software Version 0.9 (01/31/2014)

•	Performance optimizations 
•	Initial DMC support 
•	Dynamic Status screen 
•	Sahara + USB improvements 
•	Initial incorporation of dbus for script interface (a sample perl script at /usr/QXDM/Javascript/test_dbus.pl once installed) 
•	Initial Command Bar support 
•	Installer improvements

QXDM Professional Software Base Version 0.8 (12/17/2013)

•	Added QXDM Installer to make it easy for the installation.
•	Added Sahara feature to allow crash dump downloading.
•	Added Qshrink V3 and F3/Debug message parsing support
•	Made graphic display enhancements and performance optimizations. More LTE/TDSCDMA graphic displays added.
•	Added basic automation scripting interface support. 

QXDM Professional Software Version 0.7 (11/14/2013)
•	Added graphic displays feature. Currently have three graphic displays working: 1). LTE Mac UL Throughput. 2). LET Video DL RTP Jitter 3). TDSCDMA Power. 
•	Nv Item Browser.
•	Added icons for toolbar buttons to allow easy access to core functionality like "Connect to device", "Open ISF",  "Open Filtered View” …
•	Improved the Replay Dialog. 

QXDM Professional Software Version 0.6 (10/11/2013)

•	Added Filtered View feature. This allow user to turn on Log/event/messages … that interested and communicate with the device. We also support filtering result when opening an ISF.
•	Supported HTML displays. Most of the LTE and TDSCDMA HTML displays are done. You can try these out when replaying ISFs.
•	Added toolbar buttons for easy access to core functionality like "Connect to device", "Open ISF",  "Open Filtered View" ….
•	Added the color to the texts similar to the Windows version.
•	Implemented the replay logic, and linked the replay result to the Item View.

QXDM Professional Software Version 0.5 (10/11/2013)

•	Added Filtered View feature. This allow user to turn on Log/event/messages … that interested and communicate with the device. We also support filtering result when opening an ISF.
•	Supported HTML displays. Most of the LTE and TDSCDMA HTML displays are done. You can try these out when replaying ISFs.
•	Added toolbar buttons for easy access to core functionality like "Connect to device", "Open ISF",  "Open Filtered View" ….
•	Added the color to the texts similar to the Windows version.
•	Implemented the replay logic, and linked the replay result to the Item View.

QXDM Professional Software Version 0.4  (08/08/2013)
•	Initial testing build relea